Model {
  Name			  "F3005"
  Version		  7.8
  MdlSubVersion		  0
  GraphicalInterface {
    NumRootInports	    0
    NumRootOutports	    0
    ParameterArgumentNames  ""
    ComputedModelVersion    "1.28"
    NumModelReferences	    0
    NumTestPointedSignals   0
  }
  SavedCharacterEncoding  "windows-1252"
  SaveDefaultBlockParams  on
  ScopeRefreshTime	  0.035000
  OverrideScopeRefreshTime on
  DisableAllScopes	  off
  DataTypeOverride	  "UseLocalSettings"
  DataTypeOverrideAppliesTo "AllNumericTypes"
  MinMaxOverflowLogging	  "UseLocalSettings"
  MinMaxOverflowArchiveMode "Overwrite"
  FPTRunName		  "Run 1"
  MaxMDLFileLineLength	  120
  UserBdParams		  "PhysicalModelingChecksum;PhysicalModelingParameterChecksum;PhysicalModelingProducts"
  PhysicalModelingChecksum "4266331033"
  PhysicalModelingParameterChecksum "1680876564"
  PhysicalModelingProducts "SimElectronics|SimMechanics|Simscape"
  Created		  "Wed May 29 07:50:01 2013"
  Creator		  "Cedrick"
  UpdateHistory		  "UpdateHistoryNever"
  ModifiedByFormat	  "%<Auto>"
  LastModifiedBy	  "Bruno"
  ModifiedDateFormat	  "%<Auto>"
  LastModifiedDate	  "Sun May 03 12:11:23 2015"
  RTWModifiedTimeStamp	  352555858
  ModelVersionFormat	  "1.%<AutoIncrement:28>"
  ConfigurationManager	  "None"
  SampleTimeColors	  off
  SampleTimeAnnotations	  off
  LibraryLinkDisplay	  "none"
  WideLines		  off
  ShowLineDimensions	  off
  ShowPortDataTypes	  off
  ShowDesignRanges	  off
  ShowLoopsOnError	  on
  IgnoreBidirectionalLines off
  ShowStorageClass	  off
  ShowTestPointIcons	  on
  ShowSignalResolutionIcons on
  ShowViewerIcons	  on
  SortedOrder		  off
  ExecutionContextIcon	  off
  ShowLinearizationAnnotations on
  BlockNameDataTip	  off
  BlockParametersDataTip  off
  BlockDescriptionStringDataTip	off
  ToolBar		  on
  StatusBar		  on
  BrowserShowLibraryLinks off
  BrowserLookUnderMasks	  off
  SimulationMode	  "normal"
  LinearizationMsg	  "none"
  Profile		  off
  ParamWorkspaceSource	  "MATLABWorkspace"
  AccelSystemTargetFile	  "accel.tlc"
  AccelTemplateMakefile	  "accel_default_tmf"
  AccelMakeCommand	  "make_rtw"
  TryForcingSFcnDF	  off
  RecordCoverage	  off
  CovPath		  "/"
  CovSaveName		  "covdata"
  CovMetricSettings	  "dw"
  CovNameIncrementing	  off
  CovHtmlReporting	  on
  CovForceBlockReductionOff on
  covSaveCumulativeToWorkspaceVar on
  CovSaveSingleToWorkspaceVar on
  CovCumulativeVarName	  "covCumulativeData"
  CovCumulativeReport	  off
  CovReportOnPause	  on
  CovModelRefEnable	  "Off"
  CovExternalEMLEnable	  off
  ExtModeBatchMode	  off
  ExtModeEnableFloating	  on
  ExtModeTrigType	  "manual"
  ExtModeTrigMode	  "normal"
  ExtModeTrigPort	  "1"
  ExtModeTrigElement	  "any"
  ExtModeTrigDuration	  1000
  ExtModeTrigDurationFloating "auto"
  ExtModeTrigHoldOff	  0
  ExtModeTrigDelay	  0
  ExtModeTrigDirection	  "rising"
  ExtModeTrigLevel	  0
  ExtModeArchiveMode	  "off"
  ExtModeAutoIncOneShot	  off
  ExtModeIncDirWhenArm	  off
  ExtModeAddSuffixToVar	  off
  ExtModeWriteAllDataToWs off
  ExtModeArmWhenConnect	  on
  ExtModeSkipDownloadWhenConnect off
  ExtModeLogAll		  on
  ExtModeAutoUpdateStatusClock on
  BufferReuse		  on
  ShowModelReferenceBlockVersion off
  ShowModelReferenceBlockIO off
  Array {
    Type		    "Handle"
    Dimension		    1
    Simulink.ConfigSet {
      $ObjectID		      1
      Version		      "1.11.1"
      Array {
	Type			"Handle"
	Dimension		9
	Simulink.SolverCC {
	  $ObjectID		  2
	  Version		  "1.11.1"
	  StartTime		  "0.0"
	  StopTime		  "0.5"
	  AbsTol		  "auto"
	  FixedStep		  "auto"
	  InitialStep		  "auto"
	  MaxNumMinSteps	  "-1"
	  MaxOrder		  5
	  ZcThreshold		  "auto"
	  ConsecutiveZCsStepRelTol "10*128*eps"
	  MaxConsecutiveZCs	  "1000"
	  ExtrapolationOrder	  4
	  NumberNewtonIterations  1
	  MaxStep		  "auto"
	  MinStep		  "auto"
	  MaxConsecutiveMinStep	  "1"
	  RelTol		  "1e-3"
	  SolverMode		  "Auto"
	  ConcurrentTasks	  off
	  Solver		  "ode15s"
	  SolverName		  "ode15s"
	  SolverJacobianMethodControl "auto"
	  ShapePreserveControl	  "DisableAll"
	  ZeroCrossControl	  "UseLocalSettings"
	  ZeroCrossAlgorithm	  "Nonadaptive"
	  AlgebraicLoopSolver	  "TrustRegion"
	  SolverResetMethod	  "Fast"
	  PositivePriorityOrder	  off
	  AutoInsertRateTranBlk	  off
	  SampleTimeConstraint	  "Unconstrained"
	  InsertRTBMode		  "Whenever possible"
	}
	Simulink.DataIOCC {
	  $ObjectID		  3
	  Version		  "1.11.1"
	  Decimation		  "1"
	  ExternalInput		  "[t, u]"
	  FinalStateName	  "xFinal"
	  InitialState		  "xInitial"
	  LimitDataPoints	  on
	  MaxDataPoints		  "1000"
	  LoadExternalInput	  off
	  LoadInitialState	  off
	  SaveFinalState	  off
	  SaveCompleteFinalSimState off
	  SaveFormat		  "Array"
	  SignalLoggingSaveFormat "ModelDataLogs"
	  SaveOutput		  on
	  SaveState		  off
	  SignalLogging		  on
	  DSMLogging		  on
	  InspectSignalLogs	  off
	  SaveTime		  on
	  ReturnWorkspaceOutputs  off
	  StateSaveName		  "xout"
	  TimeSaveName		  "tout"
	  OutputSaveName	  "yout"
	  SignalLoggingName	  "logsout"
	  DSMLoggingName	  "dsmout"
	  OutputOption		  "RefineOutputTimes"
	  OutputTimes		  "[]"
	  ReturnWorkspaceOutputsName "out"
	  Refine		  "1"
	}
	Simulink.OptimizationCC {
	  $ObjectID		  4
	  Version		  "1.11.1"
	  Array {
	    Type		    "Cell"
	    Dimension		    8
	    Cell		    "BooleansAsBitfields"
	    Cell		    "PassReuseOutputArgsAs"
	    Cell		    "PassReuseOutputArgsThreshold"
	    Cell		    "ZeroExternalMemoryAtStartup"
	    Cell		    "ZeroInternalMemoryAtStartup"
	    Cell		    "OptimizeModelRefInitCode"
	    Cell		    "NoFixptDivByZeroProtection"
	    Cell		    "UseSpecifiedMinMax"
	    PropName		    "DisabledProps"
	  }
	  BlockReduction	  on
	  BooleanDataType	  on
	  ConditionallyExecuteInputs on
	  InlineParams		  off
	  UseIntDivNetSlope	  off
	  UseFloatMulNetSlope	  off
	  UseSpecifiedMinMax	  off
	  InlineInvariantSignals  off
	  OptimizeBlockIOStorage  on
	  BufferReuse		  on
	  EnhancedBackFolding	  off
	  StrengthReduction	  off
	  ExpressionFolding	  on
	  BooleansAsBitfields	  off
	  BitfieldContainerType	  "uint_T"
	  EnableMemcpy		  on
	  MemcpyThreshold	  64
	  PassReuseOutputArgsAs	  "Structure reference"
	  ExpressionDepthLimit	  2147483647
	  FoldNonRolledExpr	  on
	  LocalBlockOutputs	  on
	  RollThreshold		  5
	  SystemCodeInlineAuto	  off
	  StateBitsets		  off
	  DataBitsets		  off
	  UseTempVars		  off
	  ZeroExternalMemoryAtStartup on
	  ZeroInternalMemoryAtStartup on
	  InitFltsAndDblsToZero	  off
	  NoFixptDivByZeroProtection off
	  EfficientFloat2IntCast  off
	  EfficientMapNaN2IntZero on
	  OptimizeModelRefInitCode off
	  LifeSpan		  "inf"
	  MaxStackSize		  "Inherit from target"
	  BufferReusableBoundary  on
	  SimCompilerOptimization "Off"
	  AccelVerboseBuild	  off
	  AccelParallelForEachSubsystem	on
	}
	Simulink.DebuggingCC {
	  $ObjectID		  5
	  Version		  "1.11.1"
	  RTPrefix		  "error"
	  ConsistencyChecking	  "none"
	  ArrayBoundsChecking	  "none"
	  SignalInfNanChecking	  "none"
	  SignalRangeChecking	  "none"
	  ReadBeforeWriteMsg	  "UseLocalSettings"
	  WriteAfterWriteMsg	  "UseLocalSettings"
	  WriteAfterReadMsg	  "UseLocalSettings"
	  AlgebraicLoopMsg	  "warning"
	  ArtificialAlgebraicLoopMsg "warning"
	  SaveWithDisabledLinksMsg "warning"
	  SaveWithParameterizedLinksMsg	"warning"
	  CheckSSInitialOutputMsg on
	  UnderspecifiedInitializationDetection	"Classic"
	  MergeDetectMultiDrivingBlocksExec "none"
	  CheckExecutionContextPreStartOutputMsg off
	  CheckExecutionContextRuntimeOutputMsg	off
	  SignalResolutionControl "UseLocalSettings"
	  BlockPriorityViolationMsg "warning"
	  MinStepSizeMsg	  "warning"
	  TimeAdjustmentMsg	  "none"
	  MaxConsecutiveZCsMsg	  "error"
	  MaskedZcDiagnostic	  "warning"
	  IgnoredZcDiagnostic	  "warning"
	  SolverPrmCheckMsg	  "warning"
	  InheritedTsInSrcMsg	  "warning"
	  DiscreteInheritContinuousMsg "warning"
	  MultiTaskDSMMsg	  "error"
	  MultiTaskCondExecSysMsg "error"
	  MultiTaskRateTransMsg	  "error"
	  SingleTaskRateTransMsg  "none"
	  TasksWithSamePriorityMsg "warning"
	  SigSpecEnsureSampleTimeMsg "warning"
	  CheckMatrixSingularityMsg "none"
	  IntegerOverflowMsg	  "warning"
	  Int32ToFloatConvMsg	  "warning"
	  ParameterDowncastMsg	  "error"
	  ParameterOverflowMsg	  "error"
	  ParameterUnderflowMsg	  "none"
	  ParameterPrecisionLossMsg "warning"
	  ParameterTunabilityLossMsg "warning"
	  FixptConstUnderflowMsg  "none"
	  FixptConstOverflowMsg	  "none"
	  FixptConstPrecisionLossMsg "none"
	  UnderSpecifiedDataTypeMsg "none"
	  UnnecessaryDatatypeConvMsg "none"
	  VectorMatrixConversionMsg "none"
	  InvalidFcnCallConnMsg	  "error"
	  FcnCallInpInsideContextMsg "Use local settings"
	  SignalLabelMismatchMsg  "none"
	  UnconnectedInputMsg	  "warning"
	  UnconnectedOutputMsg	  "warning"
	  UnconnectedLineMsg	  "warning"
	  SFcnCompatibilityMsg	  "none"
	  FrameProcessingCompatibilityMsg "warning"
	  UniqueDataStoreMsg	  "none"
	  BusObjectLabelMismatch  "warning"
	  RootOutportRequireBusObject "warning"
	  AssertControl		  "UseLocalSettings"
	  EnableOverflowDetection off
	  ModelReferenceIOMsg	  "none"
	  ModelReferenceMultiInstanceNormalModeStructChecksumCheck "error"
	  ModelReferenceVersionMismatchMessage "none"
	  ModelReferenceIOMismatchMessage "none"
	  ModelReferenceCSMismatchMessage "none"
	  UnknownTsInhSupMsg	  "warning"
	  ModelReferenceDataLoggingMessage "warning"
	  ModelReferenceSymbolNameMessage "warning"
	  ModelReferenceExtraNoncontSigs "error"
	  StateNameClashWarn	  "warning"
	  SimStateInterfaceChecksumMismatchMsg "warning"
	  SimStateOlderReleaseMsg "error"
	  InitInArrayFormatMsg	  "warning"
	  StrictBusMsg		  "ErrorLevel1"
	  BusNameAdapt		  "WarnAndRepair"
	  NonBusSignalsTreatedAsBus "none"
	  LoggingUnavailableSignals "error"
	  BlockIODiagnostic	  "none"
	  SFUnusedDataAndEventsDiag "warning"
	  SFUnexpectedBacktrackingDiag "warning"
	  SFInvalidInputDataAccessInChartInitDiag "warning"
	  SFNoUnconditionalDefaultTransitionDiag "warning"
	  SFTransitionOutsideNaturalParentDiag "warning"
	  SFUnconditionalTransitionShadowingDiag "warning"
	}
	Simulink.HardwareCC {
	  $ObjectID		  6
	  Version		  "1.11.1"
	  ProdBitPerChar	  8
	  ProdBitPerShort	  16
	  ProdBitPerInt		  32
	  ProdBitPerLong	  32
	  ProdBitPerFloat	  32
	  ProdBitPerDouble	  64
	  ProdBitPerPointer	  32
	  ProdLargestAtomicInteger "Char"
	  ProdLargestAtomicFloat  "None"
	  ProdIntDivRoundTo	  "Undefined"
	  ProdEndianess		  "Unspecified"
	  ProdWordSize		  32
	  ProdShiftRightIntArith  on
	  ProdHWDeviceType	  "32-bit Generic"
	  TargetBitPerChar	  8
	  TargetBitPerShort	  16
	  TargetBitPerInt	  32
	  TargetBitPerLong	  32
	  TargetBitPerFloat	  32
	  TargetBitPerDouble	  64
	  TargetBitPerPointer	  32
	  TargetLargestAtomicInteger "Char"
	  TargetLargestAtomicFloat "None"
	  TargetShiftRightIntArith on
	  TargetIntDivRoundTo	  "Undefined"
	  TargetEndianess	  "Unspecified"
	  TargetWordSize	  32
	  TargetTypeEmulationWarnSuppressLevel 0
	  TargetPreprocMaxBitsSint 32
	  TargetPreprocMaxBitsUint 32
	  TargetHWDeviceType	  "Specified"
	  TargetUnknown		  off
	  ProdEqTarget		  on
	}
	Simulink.ModelReferenceCC {
	  $ObjectID		  7
	  Version		  "1.11.1"
	  UpdateModelReferenceTargets "IfOutOfDateOrStructuralChange"
	  CheckModelReferenceTargetMessage "error"
	  EnableParallelModelReferenceBuilds off
	  ParallelModelReferenceErrorOnInvalidPool on
	  ParallelModelReferenceMATLABWorkerInit "None"
	  ModelReferenceNumInstancesAllowed "Multi"
	  PropagateVarSize	  "Infer from blocks in model"
	  ModelReferencePassRootInputsByReference on
	  ModelReferenceMinAlgLoopOccurrences off
	  PropagateSignalLabelsOutOfModel off
	  SupportModelReferenceSimTargetCustomCode off
	}
	Simulink.SFSimCC {
	  $ObjectID		  8
	  Version		  "1.11.1"
	  SFSimEnableDebug	  on
	  SFSimOverflowDetection  on
	  SFSimEcho		  on
	  SimBlas		  on
	  SimCtrlC		  on
	  SimExtrinsic		  on
	  SimIntegrity		  on
	  SimUseLocalCustomCode	  off
	  SimParseCustomCode	  on
	  SimBuildMode		  "sf_incremental_build"
	}
	Simulink.RTWCC {
	  $BackupClass		  "Simulink.RTWCC"
	  $ObjectID		  9
	  Version		  "1.11.1"
	  Array {
	    Type		    "Cell"
	    Dimension		    15
	    Cell		    "IncludeHyperlinkInReport"
	    Cell		    "GenerateTraceInfo"
	    Cell		    "GenerateTraceReport"
	    Cell		    "GenerateTraceReportSl"
	    Cell		    "GenerateTraceReportSf"
	    Cell		    "GenerateTraceReportEml"
	    Cell		    "PortableWordSizes"
	    Cell		    "GenerateWebview"
	    Cell		    "GenerateCodeMetricsReport"
	    Cell		    "GenerateCodeReplacementReport"
	    Cell		    "GenerateErtSFunction"
	    Cell		    "CreateSILPILBlock"
	    Cell		    "CodeExecutionProfiling"
	    Cell		    "CodeProfilingSaveOptions"
	    Cell		    "CodeProfilingInstrumentation"
	    PropName		    "DisabledProps"
	  }
	  SystemTargetFile	  "grt.tlc"
	  GenCodeOnly		  off
	  MakeCommand		  "make_rtw"
	  GenerateMakefile	  on
	  TemplateMakefile	  "grt_default_tmf"
	  GenerateReport	  off
	  SaveLog		  off
	  RTWVerbose		  on
	  RetainRTWFile		  off
	  ProfileTLC		  off
	  TLCDebug		  off
	  TLCCoverage		  off
	  TLCAssert		  off
	  ProcessScriptMode	  "Default"
	  ConfigurationMode	  "Optimized"
	  ConfigAtBuild		  off
	  RTWUseLocalCustomCode	  off
	  RTWUseSimCustomCode	  off
	  IncludeHyperlinkInReport off
	  LaunchReport		  off
	  TargetLang		  "C"
	  IncludeBusHierarchyInRTWFileBlockHierarchyMap	off
	  IncludeERTFirstTime	  off
	  GenerateTraceInfo	  off
	  GenerateTraceReport	  off
	  GenerateTraceReportSl	  off
	  GenerateTraceReportSf	  off
	  GenerateTraceReportEml  off
	  GenerateCodeInfo	  off
	  GenerateSLWebview	  off
	  GenerateCodeMetricsReport off
	  RTWCompilerOptimization "Off"
	  CheckMdlBeforeBuild	  "Off"
	  CustomRebuildMode	  "OnUpdate"
	  Array {
	    Type		    "Handle"
	    Dimension		    2
	    Simulink.CodeAppCC {
	      $ObjectID		      10
	      Version		      "1.11.1"
	      Array {
		Type			"Cell"
		Dimension		22
		Cell			"IgnoreCustomStorageClasses"
		Cell			"IgnoreTestpoints"
		Cell			"InsertBlockDesc"
		Cell			"InsertPolySpaceComments"
		Cell			"SFDataObjDesc"
		Cell			"MATLABFcnDesc"
		Cell			"SimulinkDataObjDesc"
		Cell			"DefineNamingRule"
		Cell			"SignalNamingRule"
		Cell			"ParamNamingRule"
		Cell			"InternalIdentifier"
		Cell			"InlinedPrmAccess"
		Cell			"CustomSymbolStr"
		Cell			"CustomSymbolStrGlobalVar"
		Cell			"CustomSymbolStrType"
		Cell			"CustomSymbolStrField"
		Cell			"CustomSymbolStrFcn"
		Cell			"CustomSymbolStrFcnArg"
		Cell			"CustomSymbolStrBlkIO"
		Cell			"CustomSymbolStrTmpVar"
		Cell			"CustomSymbolStrMacro"
		Cell			"ReqsInCode"
		PropName		"DisabledProps"
	      }
	      ForceParamTrailComments off
	      GenerateComments	      on
	      IgnoreCustomStorageClasses on
	      IgnoreTestpoints	      off
	      IncHierarchyInIds	      off
	      MaxIdLength	      31
	      PreserveName	      off
	      PreserveNameWithParent  off
	      ShowEliminatedStatement off
	      IncAutoGenComments      off
	      SimulinkDataObjDesc     off
	      SFDataObjDesc	      off
	      MATLABFcnDesc	      off
	      IncDataTypeInIds	      off
	      MangleLength	      1
	      CustomSymbolStrGlobalVar "$R$N$M"
	      CustomSymbolStrType     "$N$R$M"
	      CustomSymbolStrField    "$N$M"
	      CustomSymbolStrFcn      "$R$N$M$F"
	      CustomSymbolStrFcnArg   "rt$I$N$M"
	      CustomSymbolStrBlkIO    "rtb_$N$M"
	      CustomSymbolStrTmpVar   "$N$M"
	      CustomSymbolStrMacro    "$R$N$M"
	      DefineNamingRule	      "None"
	      ParamNamingRule	      "None"
	      SignalNamingRule	      "None"
	      InsertBlockDesc	      off
	      InsertPolySpaceComments off
	      SimulinkBlockComments   on
	      MATLABSourceComments    off
	      EnableCustomComments    off
	      InlinedPrmAccess	      "Literals"
	      ReqsInCode	      off
	      UseSimReservedNames     off
	    }
	    Simulink.GRTTargetCC {
	      $BackupClass	      "Simulink.TargetCC"
	      $ObjectID		      11
	      Version		      "1.11.1"
	      Array {
		Type			"Cell"
		Dimension		15
		Cell			"GeneratePreprocessorConditionals"
		Cell			"IncludeMdlTerminateFcn"
		Cell			"CombineOutputUpdateFcns"
		Cell			"SuppressErrorStatus"
		Cell			"ERTCustomFileBanners"
		Cell			"GenerateSampleERTMain"
		Cell			"GenerateTestInterfaces"
		Cell			"ModelStepFunctionPrototypeControlCompliant"
		Cell			"CPPClassGenCompliant"
		Cell			"MultiInstanceERTCode"
		Cell			"PurelyIntegerCode"
		Cell			"SupportComplex"
		Cell			"SupportAbsoluteTime"
		Cell			"SupportContinuousTime"
		Cell			"SupportNonInlinedSFcns"
		PropName		"DisabledProps"
	      }
	      TargetFcnLib	      "ansi_tfl_table_tmw.mat"
	      TargetLibSuffix	      ""
	      TargetPreCompLibLocation ""
	      TargetFunctionLibrary   "ANSI_C"
	      UtilityFuncGeneration   "Auto"
	      ERTMultiwordTypeDef     "System defined"
	      CodeExecutionProfiling  off
	      ERTMultiwordLength      256
	      MultiwordLength	      2048
	      GenerateFullHeader      on
	      GenerateSampleERTMain   off
	      GenerateTestInterfaces  off
	      IsPILTarget	      off
	      ModelReferenceCompliant on
	      ParMdlRefBuildCompliant on
	      CompOptLevelCompliant   on
	      ConcurrentExecutionCompliant on
	      IncludeMdlTerminateFcn  on
	      GeneratePreprocessorConditionals "Disable all"
	      CombineOutputUpdateFcns on
	      CombineSignalStateStructs	off
	      SuppressErrorStatus     off
	      ERTFirstTimeCompliant   off
	      IncludeFileDelimiter    "Auto"
	      ERTCustomFileBanners    off
	      SupportAbsoluteTime     on
	      LogVarNameModifier      "rt_"
	      MatFileLogging	      on
	      MultiInstanceERTCode    off
	      SupportNonFinite	      on
	      SupportComplex	      on
	      PurelyIntegerCode	      off
	      SupportContinuousTime   on
	      SupportNonInlinedSFcns  on
	      SupportVariableSizeSignals off
	      EnableShiftOperators    on
	      ParenthesesLevel	      "Nominal"
	      PortableWordSizes	      off
	      ModelStepFunctionPrototypeControlCompliant off
	      CPPClassGenCompliant    off
	      AutosarCompliant	      off
	      UseMalloc		      off
	      ExtMode		      off
	      ExtModeStaticAlloc      off
	      ExtModeTesting	      off
	      ExtModeStaticAllocSize  1000000
	      ExtModeTransport	      0
	      ExtModeMexFile	      "ext_comm"
	      ExtModeIntrfLevel	      "Level1"
	      RTWCAPISignals	      off
	      RTWCAPIParams	      off
	      RTWCAPIStates	      off
	      RTWCAPIRootIO	      off
	      GenerateASAP2	      off
	    }
	    PropName		    "Components"
	  }
	}
	SSC.SimscapeCC {
	  $ObjectID		  12
	  Version		  "1.0"
	  Array {
	    Type		    "Cell"
	    Dimension		    1
	    Cell		    "Name"
	    PropName		    "DisabledProps"
	  }
	  Array {
	    Type		    "Handle"
	    Dimension		    1
	    MECH.SimMechanicsCC {
	      $ObjectID		      13
	      Version		      "1.11.1"
	      Name		      "SimMechanics"
	      WarnOnRedundantConstraints on
	      WarnOnSingularInitialAssembly off
	      ShowCutJoints	      off
	      VisOnUpdateDiagram      on
	      VisDuringSimulation     on
	      EnableVisSimulationTime on
	      VisSampleTime	      "0"
	      DisableBodyVisControl   off
	      ShowCG		      on
	      ShowCS		      on
	      ShowOnlyPortCS	      off
	      HighlightModel	      on
	      FramesToBeSkipped	      "0"
	      AnimationDelay	      "3"
	      RecordAVI		      off
	      CompressAVI	      on
	      AutoFitVis	      "off"
	      EnableSelection	      on
	      LastVizWinPosition      "[-1 -1 -1 -1]"
	      CamPosition	      "[0 0 0]"
	      CamTarget		      "[0 0 -1]"
	      CamUpVector	      "[0 1 0]"
	      CamHeight		      "-1"
	      CamViewAngle	      "0"
	      VisBackgroundColor      "[0.9 0.9 0.95]"
	      DefaultBodyColor	      "[1 0 0]"
	      MDLBodyVisualizationType "Convex hull from body CS locations"
	      OVRRIDBodyVisualizationType "NONE"
	    }
	    PropName		    "Components"
	  }
	  Name			  "Simscape"
	  EditingMode		  "Full"
	  ExplicitSolverDiagnosticOptions "warning"
	  InputDerivativeDiagnosticOptions "warning"
	  GlobalZcOffDiagnosticOptions "warning"
	  SimscapeLogType	  "none"
	  SimscapeLogName	  "simlog"
	  SimscapeLogDecimation	  1
	  SimscapeLogLimitData	  on
	  SimscapeLogDataHistory  5000
	}
	PropName		"Components"
      }
      Name		      "Configuration"
      CurrentDlgPage	      "Solver"
      ConfigPrmDlgPosition     [ 480, 40, 1441, 912 ] 
    }
    PropName		    "ConfigurationSets"
  }
  Simulink.ConfigSet {
    $PropName		    "ActiveConfigurationSet"
    $ObjectID		    1
  }
  BlockDefaults {
    ForegroundColor	    "black"
    BackgroundColor	    "white"
    DropShadow		    off
    NamePlacement	    "normal"
    FontName		    "Helvetica"
    FontSize		    10
    FontWeight		    "normal"
    FontAngle		    "normal"
    ShowName		    on
    BlockRotation	    0
    BlockMirror		    off
  }
  AnnotationDefaults {
    HorizontalAlignment	    "center"
    VerticalAlignment	    "middle"
    ForegroundColor	    "black"
    BackgroundColor	    "white"
    DropShadow		    off
    FontName		    "Helvetica"
    FontSize		    10
    FontWeight		    "normal"
    FontAngle		    "normal"
    UseDisplayTextAsClickCallback off
  }
  LineDefaults {
    FontName		    "Helvetica"
    FontSize		    9
    FontWeight		    "normal"
    FontAngle		    "normal"
  }
  BlockParameterDefaults {
    Block {
      BlockType		      Constant
      Value		      "1"
      VectorParams1D	      on
      SamplingMode	      "Sample based"
      OutMin		      "[]"
      OutMax		      "[]"
      OutDataTypeStr	      "Inherit: Inherit from 'Constant value'"
      LockScale		      off
      SampleTime	      "inf"
      FramePeriod	      "inf"
      PreserveConstantTs      off
    }
    Block {
      BlockType		      Demux
      Outputs		      "4"
      DisplayOption	      "none"
      BusSelectionMode	      off
    }
    Block {
      BlockType		      Gain
      Gain		      "1"
      Multiplication	      "Element-wise(K.*u)"
      ParamMin		      "[]"
      ParamMax		      "[]"
      ParamDataTypeStr	      "Inherit: Same as input"
      OutMin		      "[]"
      OutMax		      "[]"
      OutDataTypeStr	      "Inherit: Same as input"
      LockScale		      off
      RndMeth		      "Floor"
      SaturateOnIntegerOverflow	on
      SampleTime	      "-1"
    }
    Block {
      BlockType		      Inport
      Port		      "1"
      OutputFunctionCall      off
      OutMin		      "[]"
      OutMax		      "[]"
      OutDataTypeStr	      "Inherit: auto"
      LockScale		      off
      BusOutputAsStruct	      off
      PortDimensions	      "-1"
      VarSizeSig	      "Inherit"
      SampleTime	      "-1"
      SignalType	      "auto"
      SamplingMode	      "auto"
      LatchByDelayingOutsideSignal off
      LatchInputForFeedbackSignals off
      Interpolate	      on
    }
    Block {
      BlockType		      Integrator
      ExternalReset	      "none"
      InitialConditionSource  "internal"
      InitialCondition	      "0"
      LimitOutput	      off
      UpperSaturationLimit    "inf"
      LowerSaturationLimit    "-inf"
      ShowSaturationPort      off
      ShowStatePort	      off
      AbsoluteTolerance	      "auto"
      IgnoreLimit	      off
      ZeroCross		      on
      ContinuousStateAttributes	"''"
    }
    Block {
      BlockType		      Outport
      Port		      "1"
      OutMin		      "[]"
      OutMax		      "[]"
      OutDataTypeStr	      "Inherit: auto"
      LockScale		      off
      BusOutputAsStruct	      off
      PortDimensions	      "-1"
      VarSizeSig	      "Inherit"
      SampleTime	      "-1"
      SignalType	      "auto"
      SamplingMode	      "auto"
      SourceOfInitialOutputValue "Dialog"
      OutputWhenDisabled      "held"
      InitialOutput	      "[]"
    }
    Block {
      BlockType		      PMIOPort
    }
    Block {
      BlockType		      S-Function
      FunctionName	      "system"
      SFunctionModules	      "''"
      PortCounts	      "[]"
      SFunctionDeploymentMode off
    }
    Block {
      BlockType		      Scope
      ModelBased	      off
      TickLabels	      "OneTimeTick"
      ZoomMode		      "on"
      Grid		      "on"
      TimeRange		      "auto"
      YMin		      "-5"
      YMax		      "5"
      SaveToWorkspace	      off
      SaveName		      "ScopeData"
      LimitDataPoints	      on
      MaxDataPoints	      "5000"
      Decimation	      "1"
      SampleInput	      off
      SampleTime	      "-1"
    }
    Block {
      BlockType		      SubSystem
      ShowPortLabels	      "FromPortIcon"
      Permissions	      "ReadWrite"
      PermitHierarchicalResolution "All"
      TreatAsAtomicUnit	      off
      CheckFcnCallInpInsideContextMsg off
      SystemSampleTime	      "-1"
      RTWFcnNameOpts	      "Auto"
      RTWFileNameOpts	      "Auto"
      RTWMemSecFuncInitTerm   "Inherit from model"
      RTWMemSecFuncExecute    "Inherit from model"
      RTWMemSecDataConstants  "Inherit from model"
      RTWMemSecDataInternal   "Inherit from model"
      RTWMemSecDataParameters "Inherit from model"
      SimViewingDevice	      off
      DataTypeOverride	      "UseLocalSettings"
      DataTypeOverrideAppliesTo	"AllNumericTypes"
      MinMaxOverflowLogging   "UseLocalSettings"
      SFBlockType	      "NONE"
      Variant		      off
      GeneratePreprocessorConditionals off
    }
    Block {
      BlockType		      Terminator
    }
  }
  System {
    Name		    "F3005"
    Location		    [581, 104, 1749, 737]
    Open		    on
    ModelBrowserVisibility  off
    ModelBrowserWidth	    200
    ScreenColor		    "white"
    PaperOrientation	    "landscape"
    PaperPositionMode	    "auto"
    PaperType		    "A4"
    PaperUnits		    "centimeters"
    TiledPaperMargins	    [1.270000, 1.270000, 1.270000, 1.270000]
    TiledPageScale	    1
    ShowPageBoundaries	    off
    ZoomFactor		    "100"
    ReportName		    "simulink-default.rpt"
    SIDHighWatermark	    "127"
    Block {
      BlockType		      Reference
      Name		      "48V"
      SID		      "51"
      Ports		      [0, 0, 0, 0, 0, 1, 1]
      Position		      [16, 165, 44, 205]
      BlockRotation	      270
      BlockMirror	      on
      LibraryVersion	      "1.1"
      SourceBlock	      "fl_lib/Electrical/Electrical Sources/DC Voltage Source"
      SourceType	      "DC Voltage Source"
      SourceFile	      "foundation.electrical.sources.dc_voltage"
      ComponentPath	      "foundation.electrical.sources.dc_voltage"
      ComponentVariants	      "foundation.electrical.sources.dc_voltage"
      ComponentVariantNames   "dc_voltage"
      ClassName		      "dc_voltage"
      SchemaVersion	      "1"
      v0		      "48"
      v0_unit		      "V"
      i_Log		      "off"
      v_Log		      "off"
      LocalVarNames	      "|i|v"
      LocalVarDescs	      "|i|v"
      LocalVarLogging	      "[0 0]"
    }
    Block {
      BlockType		      SubSystem
      Name		      "Branche"
      SID		      "84"
      Ports		      [0, 0, 0, 0, 0, 2]
      Position		      [935, 195, 1040, 275]
      MinAlgLoopOccurrences   off
      PropExecContextOutsideSubsystem off
      RTWSystemCode	      "Auto"
      FunctionWithSeparateData off
      Opaque		      off
      RequestExecContextInheritance off
      MaskHideContents	      off
      System {
	Name			"Branche"
	Location		[624, 545, 1792, 1173]
	Open			off
	ModelBrowserVisibility	off
	ModelBrowserWidth	200
	ScreenColor		"white"
	PaperOrientation	"landscape"
	PaperPositionMode	"auto"
	PaperType		"A4"
	PaperUnits		"centimeters"
	TiledPaperMargins	[1.270000, 1.270000, 1.270000, 1.270000]
	TiledPageScale		1
	ShowPageBoundaries	off
	ZoomFactor		"100"
	Block {
	  BlockType		  Scope
	  Name			  "Angle"
	  SID			  "82"
	  Ports			  [1]
	  Position		  [430, 179, 460, 211]
	  Floating		  off
	  Location		  [85, 876, 409, 1115]
	  Open			  off
	  NumInputPorts		  "1"
	  List {
	    ListType		    AxesTitles
	    axes1		    "%<SignalLabel>"
	  }
	  List {
	    ListType		    ScopeGraphics
	    FigureColor		    "[0.5 0.5 0.5]"
	    AxesColor		    "[0 0 0]"
	    AxesTickColor	    "[1 1 1]"
	    LineColors		    "[1 1 0;1 0 1;0 1 1;1 0 0;0 1 0;0 0 1]"
	    LineStyles		    "-|-|-|-|-|-"
	    LineWidths		    "[0.5 0.5 0.5 0.5 0.5 0.5]"
	    MarkerStyles	    "none|none|none|none|none|none"
	  }
	  TimeRange		  "0.7000000000000001"
	  YMin			  "-0.2"
	  YMax			  "1.2"
	  SaveName		  "ScopeData1"
	  DataFormat		  "StructureWithTime"
	  SampleTime		  "0"
	}
	Block {
	  BlockType		  Scope
	  Name			  "Couple résistant"
	  SID			  "83"
	  Ports			  [1]
	  Position		  [240, 214, 270, 246]
	  Floating		  off
	  Location		  [45, 521, 369, 760]
	  Open			  off
	  NumInputPorts		  "1"
	  ZoomMode		  "xonly"
	  List {
	    ListType		    AxesTitles
	    axes1		    "%<SignalLabel>"
	  }
	  List {
	    ListType		    ScopeGraphics
	    FigureColor		    "[0.5 0.5 0.5]"
	    AxesColor		    "[0 0 0]"
	    AxesTickColor	    "[1 1 1]"
	    LineColors		    "[1 1 0;1 0 1;0 1 1;1 0 0;0 1 0;0 0 1]"
	    LineStyles		    "-|-|-|-|-|-"
	    LineWidths		    "[0.5 0.5 0.5 0.5 0.5 0.5]"
	    MarkerStyles	    "none|none|none|none|none|none"
	  }
	  TimeRange		  "0.7000000000000001"
	  YMin			  "-0"
	  YMax			  "100"
	  SaveName		  "ScopeData2"
	  DataFormat		  "StructureWithTime"
	  SampleTime		  "0"
	}
	Block {
	  BlockType		  Constant
	  Name			  "Epaisseur branche"
	  SID			  "91"
	  Position		  [330, 297, 375, 323]
	  BlockMirror		  on
	  Value			  "D"
	}
	Block {
	  BlockType		  Constant
	  Name			  "Force maxi"
	  SID			  "89"
	  Position		  [490, 282, 535, 308]
	  BlockMirror		  on
	  NamePlacement		  "alternate"
	  Value			  "F"
	}
	Block {
	  BlockType		  Gain
	  Name			  "Gain"
	  SID			  "90"
	  Position		  [185, 215, 215, 245]
	  Gain			  "-1"
	  ParamDataTypeStr	  "Inherit: Inherit via internal rule"
	  OutDataTypeStr	  "Inherit: Inherit via internal rule"
	  SaturateOnIntegerOverflow off
	}
	Block {
	  BlockType		  Reference
	  Name			  "Ideal Rotational Motion Sensor"
	  SID			  "75"
	  Ports			  [0, 0, 0, 0, 0, 1, 3]
	  Position		  [505, 55, 545, 95]
	  BlockRotation		  90
	  NamePlacement		  "alternate"
	  ShowName		  off
	  LibraryVersion	  "1.1"
	  SourceBlock		  "fl_lib/Mechanical/Mechanical Sensors/Ideal Rotational\nMotion Sensor"
	  SourceType		  "Ideal Rotational\nMotion Sensor"
	  SourceFile		  "foundation.mechanical.sensors.angular_velocity"
	  ComponentPath		  "foundation.mechanical.sensors.angular_velocity"
	  ComponentVariants	  "foundation.mechanical.sensors.angular_velocity"
	  ComponentVariantNames	  "angular_velocity"
	  ClassName		  "angular_velocity"
	  SchemaVersion		  "1"
	  offset		  "0"
	  offset_unit		  "rad"
	  w_Log			  "off"
	  t_Log			  "off"
	  phi_Log		  "off"
	  LocalVarNames		  "|w|t|phi"
	  LocalVarDescs		  "|w|t|phi"
	  LocalVarLogging	  "[0 0 0]"
	}
	Block {
	  BlockType		  Reference
	  Name			  "Ideal Torque Source"
	  SID			  "74"
	  Ports			  [0, 0, 0, 0, 0, 1, 2]
	  Position		  [90, 70, 130, 110]
	  BlockRotation		  90
	  ShowName		  off
	  LibraryVersion	  "1.1"
	  SourceBlock		  "fl_lib/Mechanical/Mechanical Sources/Ideal Torque Source"
	  SourceType		  "Ideal Torque Source"
	  SourceFile		  "foundation.mechanical.sources.torque"
	  ComponentPath		  "foundation.mechanical.sources.torque"
	  ComponentVariants	  "foundation.mechanical.sources.torque"
	  ComponentVariantNames	  "torque"
	  ClassName		  "torque"
	  SchemaVersion		  "1"
	  w_Log			  "off"
	  t_Log			  "off"
	  LocalVarNames		  "|w|t"
	  LocalVarDescs		  "|w|t"
	  LocalVarLogging	  "[0 0]"
	}
	Block {
	  BlockType		  Integrator
	  Name			  "Integrator"
	  SID			  "78"
	  Ports			  [1, 1]
	  Position		  [405, 120, 435, 150]
	  BlockMirror		  on
	}
	Block {
	  BlockType		  SubSystem
	  Name			  "MATLAB Function"
	  SID			  "88"
	  Ports			  [3, 1]
	  Position		  [200, 111, 270, 159]
	  BlockMirror		  on
	  LibraryVersion	  "1.32"
	  ErrorFcn		  "Stateflow.Translate.translate"
	  PermitHierarchicalResolution "ExplicitOnly"
	  TreatAsAtomicUnit	  on
	  MinAlgLoopOccurrences	  off
	  PropExecContextOutsideSubsystem off
	  RTWSystemCode		  "Auto"
	  FunctionWithSeparateData off
	  Opaque		  off
	  RequestExecContextInheritance	off
	  MaskHideContents	  off
	  SFBlockType		  "MATLAB Function"
	  System {
	    Name		    "MATLAB Function"
	    Location		    [223, 338, 826, 833]
	    Open		    off
	    ModelBrowserVisibility  off
	    ModelBrowserWidth	    200
	    ScreenColor		    "white"
	    PaperOrientation	    "landscape"
	    PaperPositionMode	    "auto"
	    PaperType		    "A4"
	    PaperUnits		    "centimeters"
	    TiledPaperMargins	    [1.270000, 1.270000, 1.270000, 1.270000]
	    TiledPageScale	    1
	    ShowPageBoundaries	    off
	    ZoomFactor		    "100"
	    SIDHighWatermark	    "102"
	    Block {
	      BlockType		      Inport
	      Name		      "u"
	      SID		      "88::92"
	      Position		      [20, 101, 40, 119]
	      IconDisplay	      "Port number"
	    }
	    Block {
	      BlockType		      Inport
	      Name		      "C"
	      SID		      "88::93"
	      Position		      [20, 136, 40, 154]
	      Port		      "2"
	      IconDisplay	      "Port number"
	    }
	    Block {
	      BlockType		      Inport
	      Name		      "e"
	      SID		      "88::94"
	      Position		      [20, 171, 40, 189]
	      Port		      "3"
	      IconDisplay	      "Port number"
	    }
	    Block {
	      BlockType		      Demux
	      Name		      " Demux "
	      SID		      "88::100"
	      Ports		      [1, 1]
	      Position		      [270, 180, 320, 220]
	      Outputs		      "1"
	    }
	    Block {
	      BlockType		      S-Function
	      Name		      " SFunction "
	      SID		      "88::99"
	      Tag		      "Stateflow S-Function F3005 2"
	      Ports		      [3, 2]
	      Position		      [180, 100, 230, 180]
	      FunctionName	      "sf_sfun"
	      PortCounts	      "[3 2]"
	      EnableBusSupport	      on
	      Port {
		PortNumber		2
		Name			"y"
		RTWStorageClass		"Auto"
		DataLoggingNameMode	"SignalName"
	      }
	    }
	    Block {
	      BlockType		      Terminator
	      Name		      " Terminator "
	      SID		      "88::102"
	      Position		      [460, 191, 480, 209]
	    }
	    Block {
	      BlockType		      Outport
	      Name		      "y"
	      SID		      "88::98"
	      Position		      [460, 101, 480, 119]
	      IconDisplay	      "Port number"
	    }
	    Line {
	      SrcBlock		      "u"
	      SrcPort		      1
	      DstBlock		      " SFunction "
	      DstPort		      1
	    }
	    Line {
	      SrcBlock		      "C"
	      SrcPort		      1
	      DstBlock		      " SFunction "
	      DstPort		      2
	    }
	    Line {
	      SrcBlock		      "e"
	      SrcPort		      1
	      DstBlock		      " SFunction "
	      DstPort		      3
	    }
	    Line {
	      Name		      "y"
	      Labels		      [0, 0]
	      SrcBlock		      " SFunction "
	      SrcPort		      2
	      DstBlock		      "y"
	      DstPort		      1
	    }
	    Line {
	      SrcBlock		      " Demux "
	      SrcPort		      1
	      DstBlock		      " Terminator "
	      DstPort		      1
	    }
	    Line {
	      SrcBlock		      " SFunction "
	      SrcPort		      1
	      DstBlock		      " Demux "
	      DstPort		      1
	    }
	  }
	}
	Block {
	  BlockType		  Reference
	  Name			  "Mechanical Rotational Reference2"
	  SID			  "76"
	  Ports			  [0, 0, 0, 0, 0, 1]
	  Position		  [530, 150, 550, 170]
	  BlockRotation		  270
	  BlockMirror		  on
	  ShowName		  off
	  LibraryVersion	  "1.1"
	  SourceBlock		  "fl_lib/Mechanical/Rotational Elements/Mechanical\nRotational Reference"
	  SourceType		  "Mechanical\nRotational Reference"
	  SourceFile		  "foundation.mechanical.rotational.reference"
	  ComponentPath		  "foundation.mechanical.rotational.reference"
	  ComponentVariants	  "foundation.mechanical.rotational.reference"
	  ComponentVariantNames	  "reference"
	  ClassName		  "reference"
	  SchemaVersion		  "1"
	  t_Log			  "off"
	  LocalVarNames		  "|t"
	  LocalVarDescs		  "|t"
	  LocalVarLogging	  "0"
	}
	Block {
	  BlockType		  Reference
	  Name			  "PS-Simulink Converter"
	  SID			  "77"
	  Ports			  [0, 1, 0, 0, 0, 1]
	  Position		  [450, 120, 480, 150]
	  BlockMirror		  on
	  ShowName		  off
	  LibraryVersion	  "1.1"
	  SourceBlock		  "nesl_utility/PS-Simulink\nConverter"
	  SourceType		  "PS-Simulink\nConverter"
	  PhysicalDomain	  "network_engine_domain"
	  LeftPortType		  "input"
	  RightPortType		  "output"
	  SubClassName		  "ps_output"
	  Unit			  "rad/s"
	  AffineConversion	  off
	}
	Block {
	  BlockType		  Reference
	  Name			  "Simulink-PS Converter"
	  SID			  "81"
	  Ports			  [2, 0, 0, 0, 0, 0, 1]
	  Position		  [140, 117, 170, 153]
	  BlockMirror		  on
	  ShowName		  off
	  LibraryVersion	  "1.1"
	  SourceBlock		  "nesl_utility/Simulink-PS\nConverter"
	  SourceType		  "Simulink-PS\nConverter"
	  PhysicalDomain	  "network_engine_domain"
	  LeftPortType		  "input"
	  RightPortType		  "output"
	  SubClassName		  "ps_input"
	  Unit			  "N*m"
	  AffineConversion	  off
	  InputFilterTimeConstant ".001"
	  UdotUserProvided	  "1"
	}
	Block {
	  BlockType		  PMIOPort
	  Name			  "Haut"
	  SID			  "85"
	  Position		  [25, 23, 55, 37]
	  Port			  "1"
	  Side			  "Left"
	}
	Block {
	  BlockType		  PMIOPort
	  Name			  "Bas"
	  SID			  "87"
	  Position		  [35, 110, 50, 140]
	  Port			  "2"
	  Side			  "Left"
	}
	Line {
	  SrcBlock		  "PS-Simulink Converter"
	  SrcPort		  1
	  DstBlock		  "Integrator"
	  DstPort		  1
	}
	Line {
	  LineType		  "Connection"
	  SrcBlock		  "Ideal Torque Source"
	  SrcPort		  RConn2
	  DstBlock		  "Bas"
	  DstPort		  RConn1
	}
	Line {
	  LineType		  "Connection"
	  SrcBlock		  "Ideal Torque Source"
	  SrcPort		  LConn1
	  Points		  [0, -25]
	  Branch {
	    ConnectType		    "DEST_SRC"
	    DstBlock		    "Haut"
	    DstPort		    RConn1
	  }
	  Branch {
	    ConnectType		    "DEST_DEST"
	    SrcBlock		    "Ideal Rotational Motion Sensor"
	    SrcPort		    LConn1
	    Points		    [0, -10; -415, 0]
	  }
	}
	Line {
	  SrcBlock		  "MATLAB Function"
	  SrcPort		  1
	  Points		  [-10, 0]
	  Branch {
	    Points		    [0, 49; -20, 0; 0, 46]
	    DstBlock		    "Gain"
	    DstPort		    1
	  }
	  Branch {
	    DstBlock		    "Simulink-PS Converter"
	    DstPort		    1
	  }
	}
	Line {
	  LineType		  "Connection"
	  SrcBlock		  "Simulink-PS Converter"
	  SrcPort		  RConn1
	  Points		  [0, -10]
	  DstBlock		  "Ideal Torque Source"
	  DstPort		  RConn1
	}
	Line {
	  SrcBlock		  "Integrator"
	  SrcPort		  1
	  Points		  [-30, 0]
	  Branch {
	    Points		    [0, -15]
	    DstBlock		    "MATLAB Function"
	    DstPort		    1
	  }
	  Branch {
	    Points		    [0, 60]
	    DstBlock		    "Angle"
	    DstPort		    1
	  }
	}
	Line {
	  LineType		  "Connection"
	  SrcBlock		  "Mechanical Rotational Reference2"
	  SrcPort		  LConn1
	  DstBlock		  "Ideal Rotational Motion Sensor"
	  DstPort		  RConn1
	}
	Line {
	  LineType		  "Connection"
	  SrcBlock		  "PS-Simulink Converter"
	  SrcPort		  LConn1
	  Points		  [30, 0]
	  DstBlock		  "Ideal Rotational Motion Sensor"
	  DstPort		  RConn2
	}
	Line {
	  SrcBlock		  "Force maxi"
	  SrcPort		  1
	  Points		  [0, -55; -148, 0; 0, -105]
	  DstBlock		  "MATLAB Function"
	  DstPort		  2
	}
	Line {
	  SrcBlock		  "Gain"
	  SrcPort		  1
	  DstBlock		  "Couple résistant"
	  DstPort		  1
	}
	Line {
	  SrcBlock		  "Epaisseur branche"
	  SrcPort		  1
	  Points		  [-19, 0; 0, -75; -21, 0]
	  DstBlock		  "MATLAB Function"
	  DstPort		  3
	}
      }
    }
    Block {
      BlockType		      Reference
      Name		      "Electrical Reference"
      SID		      "52"
      Ports		      [0, 0, 0, 0, 0, 1]
      Position		      [70, 230, 110, 270]
      BlockRotation	      270
      BlockMirror	      on
      ShowName		      off
      LibraryVersion	      "1.1"
      SourceBlock	      "fl_lib/Electrical/Electrical Elements/Electrical Reference"
      SourceType	      "Electrical Reference"
      SourceFile	      "foundation.electrical.elements.reference"
      ComponentPath	      "foundation.electrical.elements.reference"
      ComponentVariants	      "foundation.electrical.elements.reference"
      ComponentVariantNames   "reference"
      ClassName		      "reference"
      SchemaVersion	      "1"
      i_Log		      "off"
      LocalVarNames	      "|i"
      LocalVarDescs	      "|i"
      LocalVarLogging	      "0"
    }
    Block {
      BlockType		      Reference
      Name		      "Mechanical Rotational Reference"
      SID		      "33"
      Ports		      [0, 0, 0, 0, 0, 1]
      Position		      [490, 260, 510, 280]
      BlockRotation	      270
      BlockMirror	      on
      ShowName		      off
      LibraryVersion	      "1.1"
      SourceBlock	      "fl_lib/Mechanical/Rotational Elements/Mechanical\nRotational Reference"
      SourceType	      "Mechanical\nRotational Reference"
      SourceFile	      "foundation.mechanical.rotational.reference"
      ComponentPath	      "foundation.mechanical.rotational.reference"
      ComponentVariants	      "foundation.mechanical.rotational.reference"
      ComponentVariantNames   "reference"
      ClassName		      "reference"
      SchemaVersion	      "1"
      t_Log		      "off"
      LocalVarNames	      "|t"
      LocalVarDescs	      "|t"
      LocalVarLogging	      "0"
    }
    Block {
      BlockType		      Reference
      Name		      "Mechanical Rotational Reference1"
      SID		      "73"
      Ports		      [0, 0, 0, 0, 0, 1]
      Position		      [895, 320, 915, 340]
      BlockRotation	      270
      BlockMirror	      on
      ShowName		      off
      LibraryVersion	      "1.1"
      SourceBlock	      "fl_lib/Mechanical/Rotational Elements/Mechanical\nRotational Reference"
      SourceType	      "Mechanical\nRotational Reference"
      SourceFile	      "foundation.mechanical.rotational.reference"
      ComponentPath	      "foundation.mechanical.rotational.reference"
      ComponentVariants	      "foundation.mechanical.rotational.reference"
      ComponentVariantNames   "reference"
      ClassName		      "reference"
      SchemaVersion	      "1"
      t_Log		      "off"
      LocalVarNames	      "|t"
      LocalVarDescs	      "|t"
      LocalVarLogging	      "0"
    }
    Block {
      BlockType		      SubSystem
      Name		      "Motoréducteur"
      SID		      "41"
      RequirementInfo	      "{}  %GIDa_f6310b40_c8af_4236_9c0d_b603e2ac080b"
      Ports		      [0, 1, 0, 0, 0, 2, 2]
      Position		      [135, 124, 410, 236]
      BackgroundColor	      "orange"
      FontName		      "Arial"
      FontSize		      12
      FontWeight	      "bold"
      MinAlgLoopOccurrences   off
      PropExecContextOutsideSubsystem off
      RTWSystemCode	      "Auto"
      FunctionWithSeparateData off
      Opaque		      off
      RequestExecContextInheritance off
      MaskHideContents	      off
      System {
	Name			"Motoréducteur"
	Location		[644, 166, 1808, 741]
	Open			off
	ModelBrowserVisibility	off
	ModelBrowserWidth	200
	ScreenColor		"white"
	PaperOrientation	"landscape"
	PaperPositionMode	"auto"
	PaperType		"A4"
	PaperUnits		"centimeters"
	TiledPaperMargins	[1.270000, 1.270000, 1.270000, 1.270000]
	TiledPageScale		1
	ShowPageBoundaries	off
	ZoomFactor		"100"
	Block {
	  BlockType		  Scope
	  Name			  "Courant"
	  SID			  "122"
	  Ports			  [1]
	  Position		  [580, 244, 610, 276]
	  ZOrder		  -16
	  Floating		  off
	  Location		  [62, 399, 493, 688]
	  Open			  off
	  NumInputPorts		  "1"
	  List {
	    ListType		    AxesTitles
	    axes1		    "%<SignalLabel>"
	  }
	  List {
	    ListType		    ScopeGraphics
	    FigureColor		    "[0.501960784313725 0.501960784313725 0.501960784313725]"
	    AxesColor		    "[0 0 0]"
	    AxesTickColor	    "[1 1 1]"
	    LineColors		    "[1 1 0;1 0 1;0 1 1;1 0 0;0 1 0;0 0 1]"
	    LineStyles		    "-|-|-|-|-|-"
	    LineWidths		    "[0.5 0.5 0.5 0.5 0.5 0.5]"
	    MarkerStyles	    "none|none|none|none|none|none"
	  }
	  TimeRange		  "0.5"
	  YMin			  "-27.5"
	  YMax			  "0"
	  SaveName		  "ScopeData3"
	  DataFormat		  "StructureWithTime"
	  SampleTime		  "0"
	}
	Block {
	  BlockType		  Reference
	  Name			  "Current Sensor"
	  SID			  "120"
	  Ports			  [0, 0, 0, 0, 0, 1, 2]
	  Position		  [240, 250, 280, 290]
	  LibraryVersion	  "1.1"
	  SourceBlock		  "fl_lib/Electrical/Electrical Sensors/Current Sensor"
	  SourceType		  "Current Sensor"
	  SourceFile		  "foundation.electrical.sensors.current"
	  ComponentPath		  "foundation.electrical.sensors.current"
	  ComponentVariants	  "foundation.electrical.sensors.current"
	  ComponentVariantNames	  "current"
	  ClassName		  "current"
	  SchemaVersion		  "1"
	  i1_Log		  "off"
	  v1_Log		  "off"
	  LocalVarNames		  "|i1|v1"
	  LocalVarDescs		  "|i1|v1"
	  LocalVarLogging	  "[0 0]"
	}
	Block {
	  BlockType		  Reference
	  Name			  "DC Motor"
	  SID			  "123"
	  Ports			  [0, 0, 0, 0, 0, 2, 2]
	  Position		  [315, 140, 395, 190]
	  BlockRotation		  270
	  BlockMirror		  on
	  LibraryVersion	  "1.1"
	  SourceBlock		  "elec_lib/Actuators & Drivers/Rotational Actuators/DC Motor"
	  SourceType		  "DC Motor"
	  SourceFile		  "elec.actuators.rotational.dc_motor"
	  ComponentPath		  "elec.actuators.rotational.dc_motor"
	  ComponentVariants	  "elec.actuators.rotational.dc_motor"
	  ComponentVariantNames	  "dc_motor"
	  ClassName		  "dc_motor"
	  SchemaVersion		  "1"
	  parameterization	  "1"
	  parameterization_unit	  "1"
	  Ra			  "1.6"
	  Ra_unit		  "Ohm"
	  La			  "0.24"
	  La_unit		  "mH"
	  emf_or_torque		  "2"
	  emf_or_torque_unit	  "1"
	  Kv			  "7.2e-5"
	  Kv_unit		  "V/rpm"
	  Ki			  "38.7"
	  Ki_unit		  "mN*m/A"
	  T_stall		  "2.4e-4"
	  T_stall_unit		  "N*m"
	  w_max			  "1.91e+4"
	  w_max_unit		  "rpm"
	  w_rated		  "1.5e+4"
	  w_rated_unit		  "rpm"
	  P_rated		  "0.08"
	  P_rated_unit		  "W"
	  V_rated		  "1.5"
	  V_rated_unit		  "V"
	  J			  "33e-7"
	  J_unit		  "kg*m^2"
	  lam_param		  "2"
	  lam_param_unit	  "1"
	  lam			  "0"
	  lam_unit		  "N*m/(rad/s)"
	  i_noload		  "0.09"
	  i_noload_unit		  "A"
	  V_i_noload		  "48"
	  V_i_noload_unit	  "V"
	  speed0		  "0"
	  speed0_unit		  "rpm"
	  current_Log		  "off"
	  voltage_Log		  "off"
	  power_Log		  "off"
	  i2r_Log		  "off"
	  torque_Log		  "off"
	  speed_Log		  "off"
	  LocalVarNames		  "|current|voltage|power|i2r|torque|speed"
	  LocalVarDescs		  "|Current (A)|Voltage (V)|Power (W)|Electrical losses (W)|Torque (Nm)|Angular speed (rad/s)"
	  LocalVarLogging	  "[0 0 0 0 0 0]"
	}
	Block {
	  BlockType		  Reference
	  Name			  "Ideal Rotational Motion Sensor"
	  SID			  "57"
	  Ports			  [0, 0, 0, 0, 0, 1, 3]
	  Position		  [615, 105, 655, 145]
	  BlockRotation		  270
	  BlockMirror		  on
	  NamePlacement		  "alternate"
	  ShowName		  off
	  LibraryVersion	  "1.1"
	  SourceBlock		  "fl_lib/Mechanical/Mechanical Sensors/Ideal Rotational\nMotion Sensor"
	  SourceType		  "Ideal Rotational\nMotion Sensor"
	  SourceFile		  "foundation.mechanical.sensors.angular_velocity"
	  ComponentPath		  "foundation.mechanical.sensors.angular_velocity"
	  ComponentVariants	  "foundation.mechanical.sensors.angular_velocity"
	  ComponentVariantNames	  "angular_velocity"
	  ClassName		  "angular_velocity"
	  SchemaVersion		  "1"
	  offset		  "0"
	  offset_unit		  "rad"
	  w_Log			  "off"
	  t_Log			  "off"
	  phi_Log		  "off"
	  LocalVarNames		  "|w|t|phi"
	  LocalVarDescs		  "|w|t|phi"
	  LocalVarLogging	  "[0 0 0]"
	}
	Block {
	  BlockType		  Reference
	  Name			  "PS-Simulink Converter"
	  SID			  "58"
	  Ports			  [0, 1, 0, 0, 0, 1]
	  Position		  [685, 155, 715, 185]
	  ShowName		  off
	  LibraryVersion	  "1.1"
	  SourceBlock		  "nesl_utility/PS-Simulink\nConverter"
	  SourceType		  "PS-Simulink\nConverter"
	  PhysicalDomain	  "network_engine_domain"
	  LeftPortType		  "input"
	  RightPortType		  "output"
	  SubClassName		  "ps_output"
	  Unit			  "rad/s"
	  AffineConversion	  off
	}
	Block {
	  BlockType		  Reference
	  Name			  "PS-Simulink Converter1"
	  SID			  "121"
	  Ports			  [0, 1, 0, 0, 0, 1]
	  Position		  [445, 245, 475, 275]
	  ShowName		  off
	  LibraryVersion	  "1.1"
	  SourceBlock		  "nesl_utility/PS-Simulink\nConverter"
	  SourceType		  "PS-Simulink\nConverter"
	  PhysicalDomain	  "network_engine_domain"
	  LeftPortType		  "input"
	  RightPortType		  "output"
	  SubClassName		  "ps_output"
	  Unit			  "A"
	  AffineConversion	  off
	}
	Block {
	  BlockType		  Reference
	  Name			  "Rotational Friction"
	  SID			  "127"
	  Ports			  [0, 0, 0, 0, 0, 1, 1]
	  Position		  [460, 105, 500, 145]
	  BlockRotation		  90
	  NamePlacement		  "alternate"
	  LibraryVersion	  "1.1"
	  SourceBlock		  "fl_lib/Mechanical/Rotational Elements/Rotational Friction"
	  SourceType		  "Rotational Friction"
	  SourceFile		  "foundation.mechanical.rotational.friction"
	  ComponentPath		  "foundation.mechanical.rotational.friction"
	  ComponentVariants	  "foundation.mechanical.rotational.friction"
	  ComponentVariantNames	  "friction"
	  ClassName		  "friction"
	  SchemaVersion		  "1"
	  brkwy_trq		  "250"
	  brkwy_trq_unit	  "mN*m"
	  Col_trq		  "20"
	  Col_trq_unit		  "mN*m"
	  visc_coef		  "0.0002"
	  visc_coef_unit	  "N*m/(rad/s)"
	  trans_coef		  "1"
	  trans_coef_unit	  "s/rad"
	  vel_thr		  "1e-4"
	  vel_thr_unit		  "rad/s"
	  t_Log			  "off"
	  w_Log			  "off"
	  LocalVarNames		  "|t|w"
	  LocalVarDescs		  "|t|w"
	  LocalVarLogging	  "[0 0]"
	}
	Block {
	  BlockType		  Reference
	  Name			  "Réducteur"
	  SID			  "42"
	  Ports			  [0, 0, 0, 0, 0, 1, 1]
	  Position		  [680, 65, 720, 105]
	  LibraryVersion	  "1.1"
	  SourceBlock		  "fl_lib/Mechanical/Mechanisms/Gear Box"
	  SourceType		  "Gear Box"
	  SourceFile		  "foundation.mechanical.mechanisms.gear_box"
	  ComponentPath		  "foundation.mechanical.mechanisms.gear_box"
	  ComponentVariants	  "foundation.mechanical.mechanisms.gear_box"
	  ComponentVariantNames	  "gear_box"
	  ClassName		  "gear_box"
	  SchemaVersion		  "1"
	  ratio			  "-17.4"
	  ratio_unit		  "1"
	  t_in_Log		  "off"
	  t_out_Log		  "off"
	  LocalVarNames		  "|t_in|t_out"
	  LocalVarDescs		  "|t_in|t_out"
	  LocalVarLogging	  "[0 0]"
	}
	Block {
	  BlockType		  PMIOPort
	  Name			  "V+"
	  SID			  "47"
	  Position		  [115, 78, 145, 92]
	  FontName		  "Arial"
	  Port			  "1"
	  Side			  "Left"
	}
	Block {
	  BlockType		  PMIOPort
	  Name			  "rotor"
	  SID			  "48"
	  Position		  [785, 78, 815, 92]
	  BlockMirror		  on
	  FontName		  "Arial"
	  Port			  "2"
	  Side			  "Right"
	}
	Block {
	  BlockType		  PMIOPort
	  Name			  "stator"
	  SID			  "49"
	  Position		  [785, 208, 815, 222]
	  BlockMirror		  on
	  FontName		  "Arial"
	  Port			  "3"
	  Side			  "Right"
	}
	Block {
	  BlockType		  PMIOPort
	  Name			  "V-"
	  SID			  "50"
	  Position		  [115, 263, 145, 277]
	  FontName		  "Arial"
	  Port			  "4"
	  Side			  "Left"
	}
	Block {
	  BlockType		  Outport
	  Name			  "Vitesse moteur"
	  SID			  "64"
	  Position		  [785, 163, 815, 177]
	  IconDisplay		  "Port number"
	}
	Line {
	  LineType		  "Connection"
	  SrcBlock		  "DC Motor"
	  SrcPort		  LConn2
	  Points		  [0, -40; 105, 0]
	  Branch {
	    ConnectType		    "DEST_SRC"
	    Points		    [155, 0]
	    Branch {
	      ConnectType	      "DEST_DEST"
	      SrcBlock		      "Ideal Rotational Motion Sensor"
	      SrcPort		      LConn1
	      Points		      [0, -5]
	    }
	    Branch {
	      ConnectType	      "DEST_SRC"
	      DstBlock		      "Réducteur"
	      DstPort		      LConn1
	    }
	  }
	  Branch {
	    ConnectType		    "DEST_SRC"
	    DstBlock		    "Rotational Friction"
	    DstPort		    LConn1
	  }
	}
	Line {
	  LineType		  "Connection"
	  SrcBlock		  "V+"
	  SrcPort		  RConn1
	  Points		  [175, 0]
	  DstBlock		  "DC Motor"
	  DstPort		  LConn1
	}
	Line {
	  LineType		  "Connection"
	  SrcBlock		  "Réducteur"
	  SrcPort		  RConn1
	  DstBlock		  "rotor"
	  DstPort		  RConn1
	}
	Line {
	  LineType		  "Connection"
	  SrcBlock		  "PS-Simulink Converter"
	  SrcPort		  LConn1
	  Points		  [-35, 0]
	  DstBlock		  "Ideal Rotational Motion Sensor"
	  DstPort		  RConn2
	}
	Line {
	  SrcBlock		  "PS-Simulink Converter"
	  SrcPort		  1
	  DstBlock		  "Vitesse moteur"
	  DstPort		  1
	}
	Line {
	  LineType		  "Connection"
	  SrcBlock		  "Current Sensor"
	  SrcPort		  RConn1
	  DstBlock		  "PS-Simulink Converter1"
	  DstPort		  LConn1
	}
	Line {
	  SrcBlock		  "PS-Simulink Converter1"
	  SrcPort		  1
	  DstBlock		  "Courant"
	  DstPort		  1
	}
	Line {
	  LineType		  "Connection"
	  SrcBlock		  "V-"
	  SrcPort		  RConn1
	  DstBlock		  "Current Sensor"
	  DstPort		  LConn1
	}
	Line {
	  LineType		  "Connection"
	  SrcBlock		  "Current Sensor"
	  SrcPort		  RConn2
	  Points		  [40, 0]
	  DstBlock		  "DC Motor"
	  DstPort		  RConn1
	}
	Line {
	  LineType		  "Connection"
	  SrcBlock		  "DC Motor"
	  SrcPort		  RConn2
	  Points		  [0, 10; 100, 0]
	  Branch {
	    ConnectType		    "DEST_SRC"
	    Points		    [145, 0]
	    Branch {
	      ConnectType	      "DEST_SRC"
	      DstBlock		      "Ideal Rotational Motion Sensor"
	      DstPort		      RConn1
	    }
	    Branch {
	      ConnectType	      "DEST_DEST"
	      SrcBlock		      "stator"
	      SrcPort		      RConn1
	      Points		      [-150, 0]
	    }
	  }
	  Branch {
	    ConnectType		    "DEST_DEST"
	    SrcBlock		    "Rotational Friction"
	    SrcPort		    RConn1
	    Points		    [0, 55; -5, 0]
	  }
	}
	Annotation {
	  Position		  [495, 117]
	}
      }
    }
    Block {
      BlockType		      SubSystem
      Name		      "Mécanisme du Sécateur"
      SID		      "30"
      Ports		      [0, 1, 0, 0, 0, 2, 1]
      Position		      [545, 133, 780, 242]
      FontSize		      12
      FontWeight	      "bold"
      MinAlgLoopOccurrences   off
      PropExecContextOutsideSubsystem off
      RTWSystemCode	      "Auto"
      FunctionWithSeparateData off
      Opaque		      off
      RequestExecContextInheritance off
      MaskHideContents	      off
      System {
	Name			"Mécanisme du Sécateur"
	Location		[773, 449, 1937, 1024]
	Open			off
	ModelBrowserVisibility	off
	ModelBrowserWidth	200
	ScreenColor		"white"
	PaperOrientation	"landscape"
	PaperPositionMode	"auto"
	PaperType		"A4"
	PaperUnits		"centimeters"
	TiledPaperMargins	[1.270000, 1.270000, 1.270000, 1.270000]
	TiledPageScale		1
	ShowPageBoundaries	off
	ZoomFactor		"100"
	Block {
	  BlockType		  Reference
	  Name			  "Carter-1"
	  SID			  "4"
	  Ports			  [0, 0, 0, 0, 0, 1, 3]
	  Position		  [410, 139, 470, 211]
	  ForegroundColor	  "[0.000000, 0.501961, 0.752941]"
	  LibraryVersion	  "1.1"
	  SourceBlock		  "mblibv1/Bodies/Body"
	  SourceType		  "Body"
	  LConnTagsString	  "CS2"
	  RConnTagsString	  "CS3|CS4|CS5"
	  UpdateFromCAD		  "on"
	  PMImportedID		  "Carter-1"
	  ClassName		  "Body"
	  DialogClass		  "MechanicalBodyBlock"
	  Mass			  "0.139318"
	  MassUnits		  "kg"
	  InertiaUnits		  "kg*m^2"
	  Inertia		  "[4.65145e-05,2.40803e-05,-1.08912e-05;2.40803e-05,0.000596421,6.12656e-07;-1.08912e-05,6.12656e-07,0.00"
	  "0624171]"
	  Shape			  "Cylinder"
	  ShapeDims		  "[1 1]"
	  ShapeUnits		  "m"
	  ShapeUse		  "false"
	  Density		  "1"
	  DensityUnits		  "kg/m^3"
	  DensityUse		  "false"
	  GraphicsMode		  "GFXFILE"
	  GraphicsFileName	  "F3005 - Carter-1.STL"
	  BodyColorSelMode	  "COLORPALETTE"
	  BodyColor		  "[0.24706 0.24706 0.24706]"
	  AttachedToCS		  "CS1"
	  CG			  "Right$CG$[-0.0612167 -0.00598572 -0.00332482]$WORLD$WORLD$m$[1 0 0;0 1 0;0 0 1]$3x3 Transform$rad$WORLD$fal"
	  "se$Carter-1::CG(AUTOGEN)"
	  WorkingFrames		  "Right$CS1$[0.000193212 -0.00179665 -0.000541267]$WORLD$WORLD$m$[1 0 0;0 1 0;0 0 1]$3x3 Transform$"
	  "rad$WORLD$false$Carter-1::CS1(AUTOGEN)#Left$CS2$[-0.0612167 -0.00598572 -0.00332482]$WORLD$WORLD$m$[1 0 0;0 1 0;0 0"
	  " 1]$3x3 Transform$rad$WORLD$true$Carter-1:-:F3005/RootPart::Carter-1(AUTOGEN)#Right$CS3$[0.0463699 -0.00179665 -0.0"
	  "00541267]$WORLD$WORLD$m$[1 0 0;0 1 0;0 0 1]$3x3 Transform$rad$WORLD$true$Carter-1:-:PignonMoteur-1::Carter-1(AUTOGE"
	  "N)#Right$CS4$[0.000193212 -0.00179665 -0.00459127]$WORLD$WORLD$m$[1 0 0;0 1 0;0 0 1]$3x3 Transform$rad$WORLD$true$C"
	  "arter-1:-:Couronne-2::Carter-1(AUTOGEN)#Right$CS5$[0.0521908 -0.00974336 -0.00504127]$WORLD$WORLD$m$[1 0 0;0 1 0;0 "
	  "0 1]$3x3 Transform$rad$WORLD$true$Carter-1:-:LameMobile-1::Carter-1(AUTOGEN)"
	  CGPos			  "[-0.0612167 -0.00598572 -0.00332482]"
	  CGRot			  "[1 0 0;0 1 0;0 0 1]"
	  CS0Pos		  "[]"
	  CS0Rot		  "[]"
	  CS1Pos		  "[0.000193212 -0.00179665 -0.000541267]"
	  CS1Rot		  "[1 0 0;0 1 0;0 0 1]"
	  CS2Pos		  "[-0.0612167 -0.00598572 -0.00332482]"
	  CS2Rot		  "[1 0 0;0 1 0;0 0 1]"
	  CS3Pos		  "[0.0463699 -0.00179665 -0.000541267]"
	  CS3Rot		  "[1 0 0;0 1 0;0 0 1]"
	  CS4Pos		  "[0.000193212 -0.00179665 -0.00459127]"
	  CS4Rot		  "[1 0 0;0 1 0;0 0 1]"
	  CS5Pos		  "[0.0521908 -0.00974336 -0.00504127]"
	  CS5Rot		  "[1 0 0;0 1 0;0 0 1]"
	  CS6Pos		  "[]"
	  CS6Rot		  "[]"
	  CS7Pos		  "[]"
	  CS7Rot		  "[]"
	  CS8Pos		  "[]"
	  CS8Rot		  "[]"
	  CS9Pos		  "[]"
	  CS9Rot		  "[]"
	  CS10Pos		  "[]"
	  CS10Rot		  "[]"
	  CS11Pos		  "[]"
	  CS11Rot		  "[]"
	  CS12Pos		  "[]"
	  CS12Rot		  "[]"
	  CS13Pos		  "[]"
	  CS13Rot		  "[]"
	  CS14Pos		  "[]"
	  CS14Rot		  "[]"
	  CS15Pos		  "[]"
	  CS15Rot		  "[]"
	  CS16Pos		  "[]"
	  CS16Rot		  "[]"
	  CS17Pos		  "[]"
	  CS17Rot		  "[]"
	  CS18Pos		  "[]"
	  CS18Rot		  "[]"
	  CS19Pos		  "[]"
	  CS19Rot		  "[]"
	  CS20Pos		  "[]"
	  CS20Rot		  "[]"
	}
	Block {
	  BlockType		  Reference
	  Name			  "Couronne-2"
	  SID			  "24"
	  Ports			  [0, 0, 0, 0, 0, 2, 1]
	  Position		  [825, 92, 885, 148]
	  LibraryVersion	  "1.1"
	  SourceBlock		  "mblibv1/Bodies/Body"
	  SourceType		  "Body"
	  LConnTagsString	  "CS3|CS4"
	  RConnTagsString	  "CS2"
	  UpdateFromCAD		  "on"
	  ClassName		  "Body"
	  DialogClass		  "MechanicalBodyBlock"
	  Mass			  "0.00765314"
	  MassUnits		  "kg"
	  InertiaUnits		  "kg*m^2"
	  Inertia		  "[1.01904e-06,-2.01858e-12,-2.76329e-15;-2.01858e-12,1.01904e-06,4.09319e-15;-2.76329e-15,4.09319e-15,1."
	  "166e-06]"
	  Shape			  "Cylinder"
	  ShapeDims		  "[1 1]"
	  ShapeUnits		  "m"
	  ShapeUse		  "false"
	  Density		  "1"
	  DensityUnits		  "kg/m^3"
	  DensityUse		  "false"
	  GraphicsMode		  "GFXFILE"
	  GraphicsFileName	  "F3005 - Couronne-2.STL"
	  BodyColorSelMode	  "COLORPALETTE"
	  BodyColor		  "[0.75294 0.75294 0.75294]"
	  AttachedToCS		  "CS1"
	  CG			  "Right$CG$[0.000193212 -0.00179665 -0.00482957]$WORLD$WORLD$m$[-0.614282 0.789087 0;-0.789087 -0.614282 0;0 "
	  "0 1]$3x3 Transform$rad$WORLD$false$none"
	  WorkingFrames		  "Right$CS1$[0.000193212 -0.00179665 -0.000541267]$WORLD$WORLD$m$[-0.614282 0.789087 0;-0.789087 -0"
	  ".614282 0;0 0 1]$3x3 Transform$rad$WORLD$false$none#Right$CS2$[0.000193212 -0.00179665 -0.00504127]$WORLD$WORLD$m$["
	  "1 0 0;0 1 0;0 0 1]$3x3 Transform$rad$WORLD$true$none#Left$CS3$[0.000193212 -0.00179665 -0.000541267-0.015]$WORLD$WO"
	  "RLD$m$[1 0 0;0 1 0;0 0 1]$3x3 Transform$rad$WORLD$true$none#Left$CS4$[0.000193212 -0.00179665 -0.00459127]$WORLD$WO"
	  "RLD$m$[1 0 0;0 1 0;0 0 1]$3x3 Transform$rad$WORLD$true$none"
	  CGPos			  "[0.000193212 -0.00179665 -0.00482957]"
	  CGRot			  "[-0.614282 0.789087 0;-0.789087 -0.614282 0;0 0 1]"
	  CS0Pos		  "[]"
	  CS0Rot		  "[]"
	  CS1Pos		  "[0.000193212 -0.00179665 -0.000541267]"
	  CS1Rot		  "[-0.614282 0.789087 0;-0.789087 -0.614282 0;0 0 1]"
	  CS2Pos		  "[0.000193212 -0.00179665 -0.00504127]"
	  CS2Rot		  "[1 0 0;0 1 0;0 0 1]"
	  CS3Pos		  "[0.000193212 -0.00179665 -0.000541267-0.015]"
	  CS3Rot		  "[1 0 0;0 1 0;0 0 1]"
	  CS4Pos		  "[0.000193212 -0.00179665 -0.00459127]"
	  CS4Rot		  "[1 0 0;0 1 0;0 0 1]"
	  CS5Pos		  "[]"
	  CS5Rot		  "[]"
	  CS6Pos		  "[]"
	  CS6Rot		  "[]"
	  CS7Pos		  "[]"
	  CS7Rot		  "[]"
	  CS8Pos		  "[]"
	  CS8Rot		  "[]"
	  CS9Pos		  "[]"
	  CS9Rot		  "[]"
	  CS10Pos		  "[]"
	  CS10Rot		  "[]"
	  CS11Pos		  "[]"
	  CS11Rot		  "[]"
	  CS12Pos		  "[]"
	  CS12Rot		  "[]"
	  CS13Pos		  "[]"
	  CS13Rot		  "[]"
	  CS14Pos		  "[]"
	  CS14Rot		  "[]"
	  CS15Pos		  "[]"
	  CS15Rot		  "[]"
	  CS16Pos		  "[]"
	  CS16Rot		  "[]"
	  CS17Pos		  "[]"
	  CS17Rot		  "[]"
	  CS18Pos		  "[]"
	  CS18Rot		  "[]"
	  CS19Pos		  "[]"
	  CS19Rot		  "[]"
	  CS20Pos		  "[]"
	  CS20Rot		  "[]"
	}
	Block {
	  BlockType		  Reference
	  Name			  "Gachette-2"
	  SID			  "6"
	  Ports			  [0, 0, 0, 0, 0, 1]
	  Position		  [395, 255, 455, 295]
	  ForegroundColor	  "[0.000000, 0.501961, 0.752941]"
	  LibraryVersion	  "1.1"
	  SourceBlock		  "mblibv1/Bodies/Body"
	  SourceType		  "Body"
	  LConnTagsString	  "CS2"
	  UpdateFromCAD		  "on"
	  PMImportedID		  "Gachette-2"
	  ClassName		  "Body"
	  DialogClass		  "MechanicalBodyBlock"
	  Mass			  "0.00674282"
	  MassUnits		  "kg"
	  InertiaUnits		  "kg*m^2"
	  Inertia		  "[2.551e-07,-4.88545e-07,-9.34204e-09;-4.88545e-07,2.46281e-06,-3.33956e-09;-9.34204e-09,-3.33956e-09,2."
	  "6048e-06]"
	  Shape			  "Cylinder"
	  ShapeDims		  "[1 1]"
	  ShapeUnits		  "m"
	  ShapeUse		  "false"
	  Density		  "1"
	  DensityUnits		  "kg/m^3"
	  DensityUse		  "false"
	  GraphicsMode		  "GFXFILE"
	  GraphicsFileName	  "F3005 - Gachette-2.STL"
	  BodyColorSelMode	  "COLORPALETTE"
	  BodyColor		  "[0.75294 0.75294 0.75294]"
	  AttachedToCS		  "CS1"
	  CG			  "Right$CG$[-0.00247866 -0.0318578 -0.000663041]$WORLD$WORLD$m$[1 0 0;0 1 0;0 0 1]$3x3 Transform$rad$WORLD$fa"
	  "lse$Gachette-2::CG(AUTOGEN)"
	  WorkingFrames		  "Right$CS1$[0.000193212 -0.00179665 -0.000601267]$WORLD$WORLD$m$[1 0 0;0 1 0;0 0 1]$3x3 Transform$"
	  "rad$WORLD$false$Gachette-2::CS1(AUTOGEN)#Left$CS2$[-0.00788947 -0.00658815 0.00152317]$WORLD$WORLD$m$[1 0 0;0 1 0;0"
	  " 0 1]$3x3 Transform$rad$WORLD$true$F3005/RootPart:-:Gachette-2::Gachette-2(AUTOGEN)"
	  CGPos			  "[-0.00247866 -0.0318578 -0.000663041]"
	  CGRot			  "[1 0 0;0 1 0;0 0 1]"
	  CS0Pos		  "[]"
	  CS0Rot		  "[]"
	  CS1Pos		  "[0.000193212 -0.00179665 -0.000601267]"
	  CS1Rot		  "[1 0 0;0 1 0;0 0 1]"
	  CS2Pos		  "[-0.00788947 -0.00658815 0.00152317]"
	  CS2Rot		  "[1 0 0;0 1 0;0 0 1]"
	  CS3Pos		  "[]"
	  CS3Rot		  "[]"
	  CS4Pos		  "[]"
	  CS4Rot		  "[]"
	  CS5Pos		  "[]"
	  CS5Rot		  "[]"
	  CS6Pos		  "[]"
	  CS6Rot		  "[]"
	  CS7Pos		  "[]"
	  CS7Rot		  "[]"
	  CS8Pos		  "[]"
	  CS8Rot		  "[]"
	  CS9Pos		  "[]"
	  CS9Rot		  "[]"
	  CS10Pos		  "[]"
	  CS10Rot		  "[]"
	  CS11Pos		  "[]"
	  CS11Rot		  "[]"
	  CS12Pos		  "[]"
	  CS12Rot		  "[]"
	  CS13Pos		  "[]"
	  CS13Rot		  "[]"
	  CS14Pos		  "[]"
	  CS14Rot		  "[]"
	  CS15Pos		  "[]"
	  CS15Rot		  "[]"
	  CS16Pos		  "[]"
	  CS16Rot		  "[]"
	  CS17Pos		  "[]"
	  CS17Rot		  "[]"
	  CS18Pos		  "[]"
	  CS18Rot		  "[]"
	  CS19Pos		  "[]"
	  CS19Rot		  "[]"
	  CS20Pos		  "[]"
	  CS20Rot		  "[]"
	}
	Block {
	  BlockType		  Reference
	  Name			  "Gear Constraint"
	  SID			  "25"
	  Ports			  [0, 0, 0, 0, 0, 1, 1]
	  Position		  [920, 95, 970, 145]
	  LibraryVersion	  "1.1"
	  SourceBlock		  "mblibv1/Constraints & \nDrivers/Gear Constraint"
	  SourceType		  "Gear Constraint"
	  LConnTagsString	  "__newl0"
	  RConnTagsString	  "__newr0"
	  UpdateFromCAD		  "off"
	  ClassName		  "GearConstraint"
	  DialogClass		  "GearConstraint"
	  NumSAPorts		  "0"
	  BaseRadius		  "0.00676302778"
	  BaseRadiusUnits	  "m"
	  FollowerRadius	  "0.045838297"
	  FollowerRadiusUnits	  "m"
	}
	Block {
	  BlockType		  Reference
	  Name			  "Gear Constraint1"
	  SID			  "23"
	  Ports			  [0, 0, 0, 0, 0, 1, 1]
	  Position		  [730, 45, 780, 95]
	  LibraryVersion	  "1.1"
	  SourceBlock		  "mblibv1/Constraints & \nDrivers/Gear Constraint"
	  SourceType		  "Gear Constraint"
	  LConnTagsString	  "__newl0"
	  RConnTagsString	  "__newr0"
	  UpdateFromCAD		  "off"
	  ClassName		  "GearConstraint"
	  DialogClass		  "GearConstraint"
	  NumSAPorts		  "0"
	  BaseRadius		  "0.015"
	  BaseRadiusUnits	  "m"
	  FollowerRadius	  "0.045"
	  FollowerRadiusUnits	  "m"
	}
	Block {
	  BlockType		  Reference
	  Name			  "Joint Sensor"
	  SID			  "54"
	  Ports			  [0, 1, 0, 0, 0, 1]
	  Position		  [675, 265, 715, 305]
	  LibraryVersion	  "1.1"
	  SourceBlock		  "mblibv1/Sensors & \nActuators/Joint Sensor"
	  SourceType		  "Joint Sensor"
	  UpdateFromCAD		  "off"
	  PhysicalDomain	  "Mechanical"
	  PortType		  "blob"
	  Muxed			  "on"
	  Pose			  "off"
	  Angle			  "off"
	  AngleUnits		  "rad"
	  ArcVelocity		  "on"
	  ArcVelocityUnits	  "rad/s"
	  ArcAcceleration	  "off"
	  ArcAccelerationUnits	  "deg/s^2"
	  CoordPosition		  "on"
	  CoordPositionUnits	  "m"
	  Velocity		  "off"
	  VelocityUnits		  "m/s"
	  Acceleration		  "off"
	  AccelerationUnits	  "m/s^2"
	  Quaternion		  "on"
	  QuaternionDT		  "off"
	  QuaternionDDT		  "off"
	  QuaternionUnits	  "off"
	  OutputVector		  "[1]"
	  ActiveIO		  "on"
	  Width			  "1"
	  ClassName		  "JointSensor"
	  DialogClass		  "MechanicalSensorBlock"
	  Primitive		  "R1"
	  Force			  "off"
	  ForceUnits		  "N"
	  Torque		  "off"
	  TorqueUnits		  "N*m"
	  ReferenceFrame	  "Absolute (World)"
	  ReactionSensedSide	  "Base"
	  ReactionReferenceFrame  "Absolute (World)"
	  ReactionForce		  "off"
	  ReactionForceUnits	  "N"
	  ReactionMoment	  "off"
	  ReactionMomentUnits	  "N*m"
	}
	Block {
	  BlockType		  Reference
	  Name			  "LameMobile-1"
	  SID			  "26"
	  Ports			  [0, 0, 0, 0, 0, 2]
	  Position		  [1030, 137, 1090, 193]
	  LibraryVersion	  "1.1"
	  SourceBlock		  "mblibv1/Bodies/Body"
	  SourceType		  "Body"
	  LConnTagsString	  "CS2|CS3"
	  UpdateFromCAD		  "on"
	  ClassName		  "Body"
	  DialogClass		  "MechanicalBodyBlock"
	  Mass			  "0.0159957"
	  MassUnits		  "kg"
	  InertiaUnits		  "kg*m^2"
	  Inertia		  "[1.46396e-06,-9.07103e-07,1.57256e-07;-9.07103e-07,9.12258e-06,-3.0036e-08;1.57256e-07,-3.0036e-08,9.38"
	  "956e-06]"
	  Shape			  "Cylinder"
	  ShapeDims		  "[1 1]"
	  ShapeUnits		  "m"
	  ShapeUse		  "false"
	  Density		  "1"
	  DensityUnits		  "kg/m^3"
	  DensityUse		  "false"
	  GraphicsMode		  "GFXFILE"
	  GraphicsFileName	  "F3005 - LameMobile-1.STL"
	  BodyColorSelMode	  "COLORPALETTE"
	  BodyColor		  "[0.74902;0.74902;0]"
	  AttachedToCS		  "CS1"
	  CG			  "Right$CG$[0.049409 -0.00855011 0.0103283]$WORLD$WORLD$m$[0.946252 -0.323429 0;0.323429 0.946252 0;0 0 1]$3x"
	  "3 Transform$rad$WORLD$false$none"
	  WorkingFrames		  "Right$CS1$[0.000417762 -0.0190413 -0.000541267]$WORLD$WORLD$m$[0.946252 -0.323429 0;0.323429 0.94"
	  "6252 0;0 0 1]$3x3 Transform$rad$WORLD$false$none#Left$CS2$[0.0521908 -0.00974336 -0.00504127]$WORLD$WORLD$m$[1 0 0;"
	  "0 1 0;0 0 1]$3x3 Transform$rad$WORLD$true$none#Left$CS3$[0.0521908 -0.00974336 -0.00504127]$WORLD$WORLD$m$[1 0 0;0 "
	  "1 0;0 0 1]$3x3 Transform$rad$WORLD$true$none"
	  CGPos			  "[0.049409 -0.00855011 0.0103283]"
	  CGRot			  "[0.946252 -0.323429 0;0.323429 0.946252 0;0 0 1]"
	  CS0Pos		  "[]"
	  CS0Rot		  "[]"
	  CS1Pos		  "[0.000417762 -0.0190413 -0.000541267]"
	  CS1Rot		  "[0.946252 -0.323429 0;0.323429 0.946252 0;0 0 1]"
	  CS2Pos		  "[0.0521908 -0.00974336 -0.00504127]"
	  CS2Rot		  "[1 0 0;0 1 0;0 0 1]"
	  CS3Pos		  "[0.0521908 -0.00974336 -0.00504127]"
	  CS3Rot		  "[1 0 0;0 1 0;0 0 1]"
	  CS4Pos		  "[]"
	  CS4Rot		  "[]"
	  CS5Pos		  "[]"
	  CS5Rot		  "[]"
	  CS6Pos		  "[]"
	  CS6Rot		  "[]"
	  CS7Pos		  "[]"
	  CS7Rot		  "[]"
	  CS8Pos		  "[]"
	  CS8Rot		  "[]"
	  CS9Pos		  "[]"
	  CS9Rot		  "[]"
	  CS10Pos		  "[]"
	  CS10Rot		  "[]"
	  CS11Pos		  "[]"
	  CS11Rot		  "[]"
	  CS12Pos		  "[]"
	  CS12Rot		  "[]"
	  CS13Pos		  "[]"
	  CS13Rot		  "[]"
	  CS14Pos		  "[]"
	  CS14Rot		  "[]"
	  CS15Pos		  "[]"
	  CS15Rot		  "[]"
	  CS16Pos		  "[]"
	  CS16Rot		  "[]"
	  CS17Pos		  "[]"
	  CS17Rot		  "[]"
	  CS18Pos		  "[]"
	  CS18Rot		  "[]"
	  CS19Pos		  "[]"
	  CS19Rot		  "[]"
	  CS20Pos		  "[]"
	  CS20Rot		  "[]"
	}
	Block {
	  BlockType		  Reference
	  Name			  "Machine\nEnvironment"
	  SID			  "16"
	  Ports			  [0, 0, 0, 0, 0, 0, 1]
	  Position		  [45, 165, 85, 185]
	  BlockMirror		  on
	  ShowName		  off
	  LibraryVersion	  "1.1"
	  SourceBlock		  "mblibv1/Bodies/Machine\nEnvironment"
	  SourceType		  "Machine Environment"
	  PortType		  "env"
	  PhysicalDomain	  "Mechanical"
	  ClassName		  "Environment"
	  DialogTemplateClass	  "MECH.MachineEnvironment"
	  SyncWhenCopied	  "off"
	  Gravity		  "[0 -9.81 0]"
	  GravityUnits		  "m/s^2"
	  GravityAsSignal	  off
	  Dimensionality	  "Auto-detect"
	  AnalysisType		  "Forward dynamics"
	  LinearAssemblyTolerance "1e-3"
	  LinearAssemblyToleranceUnits "m"
	  AngularAssemblyTolerance "1e-3"
	  AngularAssemblyToleranceUnits	"rad"
	  ConstraintSolverType	  "Stabilizing"
	  ConstraintRelTolerance  "1e-4"
	  ConstraintAbsTolerance  "1e-4"
	  UseRobustSingularityHandling off
	  RedundancyAnalysisToleranceType "Automatically select tolerance"
	  RedundancyAnalysisTolerance "1e-14"
	  StatePerturbationType	  "Fixed"
	  PerturbationSize	  "1e-5"
	  VisualizeMachine	  on
	  BodyVisualizationType	  "Use model default body geometries"
	  BodyColorSelMode	  "Use model default"
	  DefaultBodyColor	  "[1 0 0]"
	}
	Block {
	  BlockType		  Reference
	  Name			  "PignonMoteur-1"
	  SID			  "22"
	  Ports			  [0, 0, 0, 0, 0, 1, 1]
	  Position		  [630, 50, 690, 90]
	  LibraryVersion	  "1.1"
	  SourceBlock		  "mblibv1/Bodies/Body"
	  SourceType		  "Body"
	  LConnTagsString	  "CS3"
	  RConnTagsString	  "CS2"
	  UpdateFromCAD		  "on"
	  ClassName		  "Body"
	  DialogClass		  "MechanicalBodyBlock"
	  Mass			  "0.00968789"
	  MassUnits		  "kg"
	  InertiaUnits		  "kg*m^2"
	  Inertia		  "[3.20138e-07,-2.11838e-09,-4.49693e-10;-2.11838e-09,2.71884e-07,-7.54899e-10;-4.49693e-10,-7.54899e-10,"
	  "2.75299e-07]"
	  Shape			  "Cylinder"
	  ShapeDims		  "[1 1]"
	  ShapeUnits		  "m"
	  ShapeUse		  "false"
	  Density		  "1"
	  DensityUnits		  "kg/m^3"
	  DensityUse		  "false"
	  GraphicsMode		  "GFXFILE"
	  GraphicsFileName	  "F3005 - PignonMoteur-1.STL"
	  BodyColorSelMode	  "COLORPALETTE"
	  BodyColor		  "[0.75294 0.75294 0.75294]"
	  AttachedToCS		  "CS1"
	  CG			  "Right$CG$[-0.0224102 -0.00186901 -0.000540182]$WORLD$WORLD$m$[1 0 0;0 0.974994 0.222233;0 -0.222233 0.97499"
	  "4]$3x3 Transform$rad$WORLD$false$none"
	  WorkingFrames		  "Right$CS1$[0.000693212 -0.00179665 -0.000541267]$WORLD$WORLD$m$[1 0 0;0 0.974994 0.222233;0 -0.22"
	  "2233 0.974994]$3x3 Transform$rad$WORLD$false$none#Right$CS2$[0.000193212-0.045 -0.00179665 -0.000541267]$WORLD$WORL"
	  "D$m$[1 0 0;0 1 0;0 0 1]$3x3 Transform$rad$WORLD$true$none#Left$CS3$[0.0463699 -0.00179665 -0.000541267]$WORLD$WORLD"
	  "$m$[1 0 0;0 1 0;0 0 1]$3x3 Transform$rad$WORLD$true$none"
	  CGPos			  "[-0.0224102 -0.00186901 -0.000540182]"
	  CGRot			  "[1 0 0;0 0.974994 0.222233;0 -0.222233 0.974994]"
	  CS0Pos		  "[]"
	  CS0Rot		  "[]"
	  CS1Pos		  "[0.000693212 -0.00179665 -0.000541267]"
	  CS1Rot		  "[1 0 0;0 0.974994 0.222233;0 -0.222233 0.974994]"
	  CS2Pos		  "[0.000193212-0.045 -0.00179665 -0.000541267]"
	  CS2Rot		  "[1 0 0;0 1 0;0 0 1]"
	  CS3Pos		  "[0.0463699 -0.00179665 -0.000541267]"
	  CS3Rot		  "[1 0 0;0 1 0;0 0 1]"
	  CS4Pos		  "[]"
	  CS4Rot		  "[]"
	  CS5Pos		  "[]"
	  CS5Rot		  "[]"
	  CS6Pos		  "[]"
	  CS6Rot		  "[]"
	  CS7Pos		  "[]"
	  CS7Rot		  "[]"
	  CS8Pos		  "[]"
	  CS8Rot		  "[]"
	  CS9Pos		  "[]"
	  CS9Rot		  "[]"
	  CS10Pos		  "[]"
	  CS10Rot		  "[]"
	  CS11Pos		  "[]"
	  CS11Rot		  "[]"
	  CS12Pos		  "[]"
	  CS12Rot		  "[]"
	  CS13Pos		  "[]"
	  CS13Rot		  "[]"
	  CS14Pos		  "[]"
	  CS14Rot		  "[]"
	  CS15Pos		  "[]"
	  CS15Rot		  "[]"
	  CS16Pos		  "[]"
	  CS16Rot		  "[]"
	  CS17Pos		  "[]"
	  CS17Rot		  "[]"
	  CS18Pos		  "[]"
	  CS18Rot		  "[]"
	  CS19Pos		  "[]"
	  CS19Rot		  "[]"
	  CS20Pos		  "[]"
	  CS20Rot		  "[]"
	}
	Block {
	  BlockType		  Reference
	  Name			  "Revolute"
	  SID			  "10"
	  Ports			  [0, 0, 0, 0, 0, 2, 1]
	  Position		  [540, 42, 590, 93]
	  ForegroundColor	  "[0.000000, 0.501961, 0.752941]"
	  LibraryVersion	  "1.1"
	  SourceBlock		  "mblibv1/Joints/Revolute"
	  SourceType		  "Revolute"
	  LConnTagsString	  "__newl0|SA1"
	  RConnTagsString	  "__newr0"
	  UpdateFromCAD		  "on"
	  PMImportedID		  "Carter-1:-:PignonMoteur-1"
	  NumSAPorts		  "1"
	  CutJoint		  "off"
	  MarkAsCut		  "off"
	  Primitives		  "prismatic"
	  PrimitiveProps	  "R1$World$[1,0,0]$revolute"
	  ClassName		  "Joint"
	  DialogClass		  "JointBlock"
	  R1Axis		  "[1,0,0]"
	}
	Block {
	  BlockType		  Reference
	  Name			  "Revolute - Rotational Interface"
	  SID			  "28"
	  Ports			  [0, 0, 0, 0, 0, 2, 1]
	  Position		  [390, 60, 430, 100]
	  ShowName		  off
	  LibraryVersion	  "1.1"
	  SourceBlock		  "mblibv1/Interface \nElements/Revolute -\nRotational\nInterface"
	  SourceType		  "Revolute - Rotational Interface"
	  UpdateFromCAD		  "off"
	  ClassName		  "RevoluteRotationalInterface"
	  DialogClass		  "RevoluteRotationalInterface"
	  Primitive		  "R1"
	}
	Block {
	  BlockType		  Reference
	  Name			  "Revolute - Rotational Interface1"
	  SID			  "65"
	  Ports			  [0, 0, 0, 0, 0, 2, 1]
	  Position		  [880, 250, 920, 290]
	  BlockRotation		  270
	  ShowName		  off
	  LibraryVersion	  "1.1"
	  SourceBlock		  "mblibv1/Interface \nElements/Revolute -\nRotational\nInterface"
	  SourceType		  "Revolute - Rotational Interface"
	  UpdateFromCAD		  "off"
	  ClassName		  "RevoluteRotationalInterface"
	  DialogClass		  "RevoluteRotationalInterface"
	  Primitive		  "R1"
	}
	Block {
	  BlockType		  Reference
	  Name			  "Revolute1"
	  SID			  "12"
	  Ports			  [0, 0, 0, 0, 0, 1, 1]
	  Position		  [635, 135, 685, 185]
	  ForegroundColor	  "[0.000000, 0.501961, 0.752941]"
	  LibraryVersion	  "1.1"
	  SourceBlock		  "mblibv1/Joints/Revolute"
	  SourceType		  "Revolute"
	  LConnTagsString	  "__newl0"
	  RConnTagsString	  "__newr0"
	  UpdateFromCAD		  "on"
	  PMImportedID		  "Carter-1:-:Couronne-2"
	  NumSAPorts		  "0"
	  CutJoint		  "off"
	  MarkAsCut		  "off"
	  Primitives		  "prismatic"
	  PrimitiveProps	  "R1$WORLD$[0,0,-1]$revolute"
	  ClassName		  "Joint"
	  DialogClass		  "JointBlock"
	  R1Axis		  "[0,0,-1]"
	}
	Block {
	  BlockType		  Reference
	  Name			  "Revolute2"
	  SID			  "13"
	  Ports			  [0, 0, 0, 0, 0, 2, 2]
	  Position		  [745, 202, 795, 253]
	  ForegroundColor	  "[0.000000, 0.501961, 0.752941]"
	  LibraryVersion	  "1.1"
	  SourceBlock		  "mblibv1/Joints/Revolute"
	  SourceType		  "Revolute"
	  LConnTagsString	  "__newl0|SA1"
	  RConnTagsString	  "__newr0|SA1"
	  UpdateFromCAD		  "on"
	  PMImportedID		  "Carter-1:-:LameMobile-1"
	  NumSAPorts		  "2"
	  CutJoint		  "off"
	  MarkAsCut		  "off"
	  Primitives		  "prismatic"
	  PrimitiveProps	  "R1$World$[0,0,-1]$revolute"
	  ClassName		  "Joint"
	  DialogClass		  "JointBlock"
	  R1Axis		  "[0,0,-1]"
	}
	Block {
	  BlockType		  Reference
	  Name			  "RootGround"
	  SID			  "7"
	  Ports			  [0, 0, 0, 0, 0, 1, 1]
	  Position		  [45, 205, 85, 245]
	  ForegroundColor	  "[0.000000, 0.501961, 0.752941]"
	  LibraryVersion	  "1.1"
	  UserDataPersistent	  on
	  UserData		  "DataTag0"
	  SourceBlock		  "mblibv1/Bodies/Ground"
	  SourceType		  "Ground"
	  UpdateFromCAD		  "on"
	  PMImportedID		  "RootGround"
	  LeftPortType		  "env"
	  RightPortType		  "workingframe"
	  PhysicalDomain	  "Mechanical"
	  DialogClass		  "GroundBlock"
	  ClassName		  "Ground"
	  CoordPosition		  "[-0.00788947,-0.00658815,0.00152317]"
	  CoordPositionUnits	  "m"
	  StateVectorMgrId	  "-1"
	  MachineId		  "[0 0]"
	  ShowEnvPort		  on
	}
	Block {
	  BlockType		  Reference
	  Name			  "RootPart"
	  SID			  "5"
	  Ports			  [0, 0, 0, 0, 0, 1, 2]
	  Position		  [205, 197, 265, 253]
	  ForegroundColor	  "[0.000000, 0.501961, 0.752941]"
	  LibraryVersion	  "1.1"
	  SourceBlock		  "mblibv1/Bodies/Body"
	  SourceType		  "Body"
	  LConnTagsString	  "CS3"
	  RConnTagsString	  "CS2|CS4"
	  UpdateFromCAD		  "on"
	  PMImportedID		  "F3005/RootPart"
	  ClassName		  "Body"
	  DialogClass		  "MechanicalBodyBlock"
	  Mass			  "0"
	  MassUnits		  "kg"
	  InertiaUnits		  "kg*m^2"
	  Inertia		  "[0,0,0;0,0,0;0,0,0]"
	  Shape			  "Cylinder"
	  ShapeDims		  "[1 1]"
	  ShapeUnits		  "m"
	  ShapeUse		  "false"
	  Density		  "1"
	  DensityUnits		  "kg/m^3"
	  DensityUse		  "false"
	  GraphicsMode		  "MACHINE_DEFAULT"
	  BodyColorSelMode	  "MACHINE_DEFAULT"
	  BodyColor		  "[1 0 0]"
	  AttachedToCS		  "CS1"
	  CG			  "Right$CG$[-0.00788947 -0.00658815 0.00152317]$WORLD$WORLD$m$[1 0 0;0 1 0;0 0 1]$3x3 Transform$rad$WORLD$fal"
	  "se$F3005/RootPart::CG(AUTOGEN)"
	  WorkingFrames		  "Right$CS1$[0 0 0]$WORLD$WORLD$m$[1 0 0;0 1 0;0 0 1]$3x3 Transform$rad$WORLD$false$F3005/RootPart:"
	  ":CS1(AUTOGEN)#Right$CS2$[-0.0612167 -0.00598572 -0.00332482]$WORLD$WORLD$m$[1 0 0;0 1 0;0 0 1]$3x3 Transform$rad$WO"
	  "RLD$true$Carter-1:-:F3005/RootPart::F3005/RootPart(AUTOGEN)#Left$CS3$[-0.00788947 -0.00658815 0.00152317]$WORLD$WOR"
	  "LD$m$[1 0 0;0 1 0;0 0 1]$3x3 Transform$rad$WORLD$true$F3005/RootPart:-:RootGround::F3005/RootPart(AUTOGEN)#Right$CS"
	  "4$[-0.00788947 -0.00658815 0.00152317]$WORLD$WORLD$m$[1 0 0;0 1 0;0 0 1]$3x3 Transform$rad$WORLD$true$F3005/RootPar"
	  "t:-:Gachette-2::F3005/RootPart(AUTOGEN)"
	  CGPos			  "[-0.00788947 -0.00658815 0.00152317]"
	  CGRot			  "[1 0 0;0 1 0;0 0 1]"
	  CS0Pos		  "[]"
	  CS0Rot		  "[]"
	  CS1Pos		  "[0 0 0]"
	  CS1Rot		  "[1 0 0;0 1 0;0 0 1]"
	  CS2Pos		  "[-0.0612167 -0.00598572 -0.00332482]"
	  CS2Rot		  "[1 0 0;0 1 0;0 0 1]"
	  CS3Pos		  "[-0.00788947 -0.00658815 0.00152317]"
	  CS3Rot		  "[1 0 0;0 1 0;0 0 1]"
	  CS4Pos		  "[-0.00788947 -0.00658815 0.00152317]"
	  CS4Rot		  "[1 0 0;0 1 0;0 0 1]"
	  CS5Pos		  "[]"
	  CS5Rot		  "[]"
	  CS6Pos		  "[]"
	  CS6Rot		  "[]"
	  CS7Pos		  "[]"
	  CS7Rot		  "[]"
	  CS8Pos		  "[]"
	  CS8Rot		  "[]"
	  CS9Pos		  "[]"
	  CS9Rot		  "[]"
	  CS10Pos		  "[]"
	  CS10Rot		  "[]"
	  CS11Pos		  "[]"
	  CS11Rot		  "[]"
	  CS12Pos		  "[]"
	  CS12Rot		  "[]"
	  CS13Pos		  "[]"
	  CS13Rot		  "[]"
	  CS14Pos		  "[]"
	  CS14Rot		  "[]"
	  CS15Pos		  "[]"
	  CS15Rot		  "[]"
	  CS16Pos		  "[]"
	  CS16Rot		  "[]"
	  CS17Pos		  "[]"
	  CS17Rot		  "[]"
	  CS18Pos		  "[]"
	  CS18Rot		  "[]"
	  CS19Pos		  "[]"
	  CS19Rot		  "[]"
	  CS20Pos		  "[]"
	  CS20Rot		  "[]"
	}
	Block {
	  BlockType		  Reference
	  Name			  "Weld"
	  SID			  "8"
	  Ports			  [0, 0, 0, 0, 0, 1, 1]
	  Position		  [310, 150, 360, 200]
	  ForegroundColor	  "[0.000000, 0.501961, 0.752941]"
	  LibraryVersion	  "1.1"
	  SourceBlock		  "mblibv1/Joints/Weld"
	  SourceType		  "Weld"
	  LConnTagsString	  "__newl0"
	  RConnTagsString	  "__newr0"
	  UpdateFromCAD		  "on"
	  PMImportedID		  "Carter-1:-:F3005/RootPart"
	  NumSAPorts		  "0"
	  CutJoint		  "off"
	  MarkAsCut		  "off"
	  Primitives		  "weld"
	  PrimitiveProps	  "W$WORLD$[0.57735,0.57735,0.57735]$weld"
	  ClassName		  "Joint"
	  DialogClass		  "JointBlock"
	  WAxis			  "[0.57735,0.57735,0.57735]"
	}
	Block {
	  BlockType		  Reference
	  Name			  "Weld1"
	  SID			  "27"
	  Ports			  [0, 0, 0, 0, 0, 1, 1]
	  Position		  [305, 255, 355, 305]
	  LibraryVersion	  "1.1"
	  SourceBlock		  "mblibv1/Joints/Weld"
	  SourceType		  "Weld"
	  LConnTagsString	  "__newl0"
	  RConnTagsString	  "__newr0"
	  UpdateFromCAD		  "off"
	  NumSAPorts		  "0"
	  CutJoint		  "off"
	  MarkAsCut		  "off"
	  Primitives		  "weld"
	  PrimitiveProps	  "W$World$[0 0 0]$weld"
	  ClassName		  "Joint"
	  DialogClass		  "JointBlock"
	  WAxis			  "[0 0 0]"
	}
	Block {
	  BlockType		  Reference
	  Name			  "Weld3"
	  SID			  "14"
	  Ports			  [0, 0, 0, 0, 0, 1, 1]
	  Position		  [120, 200, 170, 250]
	  ForegroundColor	  "[0.000000, 0.501961, 0.752941]"
	  LibraryVersion	  "1.1"
	  SourceBlock		  "mblibv1/Joints/Weld"
	  SourceType		  "Weld"
	  LConnTagsString	  "__newl0"
	  RConnTagsString	  "__newr0"
	  UpdateFromCAD		  "on"
	  PMImportedID		  "F3005/RootPart:-:RootGround"
	  NumSAPorts		  "0"
	  CutJoint		  "off"
	  MarkAsCut		  "off"
	  Primitives		  "weld"
	  PrimitiveProps	  "W$WORLD$[0.57735,0.57735,0.57735]$weld"
	  ClassName		  "Joint"
	  DialogClass		  "JointBlock"
	  WAxis			  "[0.57735,0.57735,0.57735]"
	}
	Block {
	  BlockType		  PMIOPort
	  Name			  "Pignon"
	  SID			  "32"
	  Position		  [275, 83, 305, 97]
	  Port			  "1"
	  Side			  "Left"
	}
	Block {
	  BlockType		  PMIOPort
	  Name			  "Bati"
	  SID			  "31"
	  Position		  [285, 18, 315, 32]
	  Port			  "2"
	  Side			  "Left"
	}
	Block {
	  BlockType		  PMIOPort
	  Name			  "Lame"
	  SID			  "66"
	  Position		  [965, 303, 995, 317]
	  BlockMirror		  on
	  NamePlacement		  "alternate"
	  Port			  "3"
	  Side			  "Right"
	}
	Block {
	  BlockType		  Outport
	  Name			  "Vitesse Lame"
	  SID			  "55"
	  Position		  [790, 288, 820, 302]
	  IconDisplay		  "Port number"
	}
	Line {
	  LineType		  "Connection"
	  SrcBlock		  "Revolute - Rotational Interface"
	  SrcPort		  LConn2
	  DstBlock		  "Pignon"
	  DstPort		  RConn1
	}
	Line {
	  LineType		  "Connection"
	  SrcBlock		  "Revolute - Rotational Interface"
	  SrcPort		  LConn1
	  Points		  [-22, 0; 0, -19]
	  Branch {
	    ConnectType		    "DEST_DEST"
	    SrcBlock		    "Revolute - Rotational Interface1"
	    SrcPort		    LConn1
	    Points		    [0, 27; -884, 0; 0, -281; 347, 0]
	  }
	  Branch {
	    ConnectType		    "DEST_SRC"
	    Points		    [0, -26]
	    DstBlock		    "Bati"
	    DstPort		    RConn1
	  }
	}
	Line {
	  LineType		  "Connection"
	  SrcBlock		  "Weld"
	  SrcPort		  RConn1
	  DstBlock		  "Carter-1"
	  DstPort		  LConn1
	}
	Line {
	  LineType		  "Connection"
	  SrcBlock		  "Carter-1"
	  SrcPort		  RConn1
	  Points		  [20, 0; 0, -95]
	  DstBlock		  "Revolute"
	  DstPort		  LConn1
	}
	Line {
	  LineType		  "Connection"
	  SrcBlock		  "RootPart"
	  SrcPort		  RConn1
	  Points		  [0, -35]
	  DstBlock		  "Weld"
	  DstPort		  LConn1
	}
	Line {
	  LineType		  "Connection"
	  SrcBlock		  "Couronne-2"
	  SrcPort		  LConn1
	  Points		  [-3, 0; 0, -35]
	  DstBlock		  "Gear Constraint1"
	  DstPort		  RConn1
	}
	Line {
	  LineType		  "Connection"
	  SrcBlock		  "Gear Constraint1"
	  SrcPort		  LConn1
	  DstBlock		  "PignonMoteur-1"
	  DstPort		  RConn1
	}
	Line {
	  LineType		  "Connection"
	  SrcBlock		  "Revolute"
	  SrcPort		  RConn1
	  DstBlock		  "PignonMoteur-1"
	  DstPort		  LConn1
	}
	Line {
	  LineType		  "Connection"
	  SrcBlock		  "Couronne-2"
	  SrcPort		  RConn1
	  DstBlock		  "Gear Constraint"
	  DstPort		  LConn1
	}
	Line {
	  LineType		  "Connection"
	  SrcBlock		  "Carter-1"
	  SrcPort		  RConn2
	  Points		  [68, 0; 0, -15]
	  DstBlock		  "Revolute1"
	  DstPort		  LConn1
	}
	Line {
	  LineType		  "Connection"
	  SrcBlock		  "Carter-1"
	  SrcPort		  RConn3
	  Points		  [93, 0; 0, 15]
	  DstBlock		  "Revolute2"
	  DstPort		  LConn1
	}
	Line {
	  LineType		  "Connection"
	  SrcBlock		  "LameMobile-1"
	  SrcPort		  LConn1
	  Points		  [-12, 0; 0, -30]
	  DstBlock		  "Gear Constraint"
	  DstPort		  RConn1
	}
	Line {
	  LineType		  "Connection"
	  SrcBlock		  "Revolute2"
	  SrcPort		  RConn1
	  Points		  [113, 0; 0, -35]
	  DstBlock		  "LameMobile-1"
	  DstPort		  LConn2
	}
	Line {
	  LineType		  "Connection"
	  SrcBlock		  "Revolute1"
	  SrcPort		  RConn1
	  Points		  [55, 0; 0, -25]
	  DstBlock		  "Couronne-2"
	  DstPort		  LConn2
	}
	Line {
	  LineType		  "Connection"
	  SrcBlock		  "Weld1"
	  SrcPort		  LConn1
	  Points		  [0, -40]
	  DstBlock		  "RootPart"
	  DstPort		  RConn2
	}
	Line {
	  LineType		  "Connection"
	  SrcBlock		  "RootGround"
	  SrcPort		  RConn1
	  DstBlock		  "Weld3"
	  DstPort		  LConn1
	}
	Line {
	  LineType		  "Connection"
	  SrcBlock		  "Weld3"
	  SrcPort		  RConn1
	  DstBlock		  "RootPart"
	  DstPort		  LConn1
	}
	Line {
	  LineType		  "Connection"
	  SrcBlock		  "Weld1"
	  SrcPort		  RConn1
	  Points		  [5, 0; 0, -5]
	  DstBlock		  "Gachette-2"
	  DstPort		  LConn1
	}
	Line {
	  LineType		  "Connection"
	  SrcBlock		  "RootGround"
	  SrcPort		  LConn1
	  Points		  [-10, 0; 0, -50]
	  DstBlock		  "Machine\nEnvironment"
	  DstPort		  RConn1
	}
	Line {
	  LineType		  "Connection"
	  SrcBlock		  "Revolute"
	  SrcPort		  LConn2
	  DstBlock		  "Revolute - Rotational Interface"
	  DstPort		  RConn1
	}
	Line {
	  LineType		  "Connection"
	  SrcBlock		  "Joint Sensor"
	  SrcPort		  LConn1
	  Points		  [0, -45]
	  DstBlock		  "Revolute2"
	  DstPort		  LConn2
	}
	Line {
	  SrcBlock		  "Joint Sensor"
	  SrcPort		  1
	  Points		  [32, 0; 0, 10]
	  DstBlock		  "Vitesse Lame"
	  DstPort		  1
	}
	Line {
	  LineType		  "Connection"
	  SrcBlock		  "Revolute - Rotational Interface1"
	  SrcPort		  RConn1
	  Points		  [0, 5]
	  DstBlock		  "Revolute2"
	  DstPort		  RConn2
	}
	Line {
	  LineType		  "Connection"
	  SrcBlock		  "Lame"
	  SrcPort		  RConn1
	  Points		  [-40, 0]
	  DstBlock		  "Revolute - Rotational Interface1"
	  DstPort		  LConn2
	}
      }
    }
    Block {
      BlockType		      Reference
      Name		      "Solver Configuration"
      SID		      "37"
      Ports		      [0, 0, 0, 0, 0, 0, 1]
      Position		      [365, 274, 410, 306]
      LibraryVersion	      "1.1"
      SourceBlock	      "nesl_utility/Solver\nConfiguration"
      SourceType	      "Solver\nConfiguration"
      PhysicalDomain	      "network_engine_domain"
      LeftPortType	      "input"
      RightPortType	      "generic"
      SubClassName	      "solver"
      DoDC		      off
      ResidualTolerance	      "1e-9"
      UseLocalSolver	      off
      LocalSolverChoice	      "NE_BACKWARD_EULER_ADVANCER"
      LocalSolverSampleTime   ".001"
      DoFixedCost	      off
      MaxNonlinIter	      "3"
      MaxModeIter	      "2"
      LinearAlgebra	      "Sparse"
      Accelerate	      off
      Profile		      off
      UseLocalSampling	      off
      DelaysMemoryBudget      "1024"
    }
    Block {
      BlockType		      Scope
      Name		      "Vitesse de rotation\nde la lame"
      SID		      "56"
      Ports		      [1]
      Position		      [890, 144, 920, 176]
      Floating		      off
      Location		      [56, 119, 380, 358]
      Open		      off
      NumInputPorts	      "1"
      ZoomMode		      "xonly"
      List {
	ListType		AxesTitles
	axes1			"%<SignalLabel>"
      }
      List {
	ListType		ScopeGraphics
	FigureColor		"[0.5 0.5 0.5]"
	AxesColor		"[0 0 0]"
	AxesTickColor		"[1 1 1]"
	LineColors		"[1 1 0;1 0 1;0 1 1;1 0 0;0 1 0;0 0 1]"
	LineStyles		"-|-|-|-|-|-"
	LineWidths		"[0.5 0.5 0.5 0.5 0.5 0.5]"
	MarkerStyles		"none|none|none|none|none|none"
      }
      TimeRange		      "0.7000000000000001"
      YMin		      "-0.5"
      YMax		      "2.5"
      DataFormat	      "StructureWithTime"
      SampleTime	      "0"
    }
    Line {
      LineType		      "Connection"
      SrcBlock		      "Solver Configuration"
      SrcPort		      RConn1
      Points		      [27, 0; 0, -75]
      Branch {
	ConnectType		"DEST_DEST"
	Points			[500, 215; -48, 0]
	Branch {
	  ConnectType		  "SRC_DEST"
	  SrcBlock		  "Mécanisme du Sécateur"
	  SrcPort		  LConn2
	  Points		  [-30, 0]
	}
	Branch {
	  ConnectType		  "SRC_SRC"
	  DstBlock		  "Mechanical Rotational Reference"
	  DstPort		  LConn1
	}
      }
      Branch {
	ConnectType		"DEST_SRC"
	DstBlock		"Motoréducteur"
	DstPort			RConn2
      }
    }
    Line {
      LineType		      "Connection"
      SrcBlock		      "Mécanisme du Sécateur"
      SrcPort		      LConn1
      Points		      [-105, 0]
      DstBlock		      "Motoréducteur"
      DstPort		      RConn1
    }
    Line {
      LineType		      "Connection"
      SrcBlock		      "48V"
      SrcPort		      LConn1
      Points		      [0, 5]
      DstBlock		      "Motoréducteur"
      DstPort		      LConn1
    }
    Line {
      LineType		      "Connection"
      SrcBlock		      "48V"
      SrcPort		      RConn1
      Points		      [0, -10; 60, 0]
      Branch {
	ConnectType		"DEST_DEST"
	SrcBlock		"Electrical Reference"
	SrcPort			LConn1
	Points			[0, -5]
      }
      Branch {
	ConnectType		"DEST_SRC"
	DstBlock		"Motoréducteur"
	DstPort			LConn2
      }
    }
    Line {
      SrcBlock		      "Mécanisme du Sécateur"
      SrcPort		      1
      DstBlock		      "Vitesse de rotation\nde la lame"
      DstPort		      1
    }
    Line {
      LineType		      "Connection"
      SrcBlock		      "Branche"
      SrcPort		      LConn1
      DstBlock		      "Mécanisme du Sécateur"
      DstPort		      RConn1
    }
    Line {
      LineType		      "Connection"
      SrcBlock		      "Branche"
      SrcPort		      LConn2
      Points		      [-15, 0]
      DstBlock		      "Mechanical Rotational Reference1"
      DstPort		      LConn1
    }
    Annotation {
      Position		      [1016, 289]
    }
  }
}
MatData {
  NumRecords		  1
  DataRecord {
    Tag			    DataTag0
    Data		    "  %)30     .    @     8    (    !          %    \"     $    F     0         1    3    $8 ,P P #  -0 O $"
    "T Z0!C &$ ;@!I ', ;0!E \"  9 !U \"  4P#I &, 80!T &4 =0!R \"\\ 4@!O &\\ = !' '( ;P!U &X 9       "
  }
}
# Finite State Machines
#
#    Stateflow Version 7.6 (R2011b) dated Aug  6 2011, 17:15:36
#
#


Stateflow {
  machine {
    id			    1
    name		    "F3005"
    created		    "29-May-2013 12:15:57"
    isLibrary		    0
    firstTarget		    11
    sfVersion		    76014001.0002
  }
  chart {
    id			    2
    name		    "Branche/MATLAB Function"
    windowPosition	    [357.12 483.496 167 391]
    viewLimits		    [0 156.75 0 153.75]
    screen		    [1 1 1280 1024 1.041666666666667]
    treeNode		    [0 3 0 0]
    firstTransition	    5
    firstJunction	    4
    viewObj		    2
    machine		    1
    ssIdHighWaterMark	    7
    decomposition	    CLUSTER_CHART
    type		    EML_CHART
    firstData		    6
    chartFileNumber	    2
    disableImplicitCasting  1
    eml {
      name		      "fcn"
    }
  }
  state {
    id			    3
    labelString		    "eML_blk_kernel()"
    position		    [18 64.5 118 66]
    fontSize		    12
    chart		    2
    treeNode		    [2 0 0 0]
    superState		    SUBCHART
    subviewer		    2
    ssIdNumber		    1
    type		    FUNC_STATE
    decomposition	    CLUSTER_STATE
    eml {
      isEML		      1
      script		      "function y = fcn(u, C, e)\n%#codegen\ni = 0.077; % angle à parcourir avant de toucher la branche\n"
      "f = 0.748; % angle à partir duquel la branche est fini de couper\nd = f-e/25*(f-i); % angle à partir duquel la b"
      "ranche est coupée\n\nif u > d\n    co = -C*0.053*sin(47)*sin((u-d)*pi/(f-d));\n    if co < 0\n        y = co;\n "
      "   else\n        y = 0;\n    end\nelse\n    y = 0;\nend"
      editorLayout	      "100 M4x1[10 257 700 500]"
    }
  }
  junction {
    id			    4
    position		    [23.5747 49.5747 7]
    chart		    2
    linkNode		    [2 0 0]
    subviewer		    2
    ssIdNumber		    3
    type		    CONNECTIVE_JUNCTION
  }
  transition {
    id			    5
    labelString		    "{eML_blk_kernel();}"
    labelPosition	    [32.125 19.875 102.544 14.964]
    fontSize		    12
    src {
      intersection	      [0 0 1 0 23.5747 14.625 0 0]
    }
    dst {
      id		      4
      intersection	      [1 0 -1 0 23.5747 42.5747 0 0]
    }
    midPoint		    [23.5747 24.9468]
    chart		    2
    linkNode		    [2 0 0]
    dataLimits		    [21.175 25.975 14.625 42.575]
    subviewer		    2
    drawStyle		    SMART
    slide {
      sticky		      BOTH_STICK
    }
    executionOrder	    1
    ssIdNumber		    2
  }
  data {
    id			    6
    ssIdNumber		    4
    name		    "u"
    linkNode		    [2 0 7]
    scope		    INPUT_DATA
    machine		    1
    props {
      array {
	size			"-1"
      }
      type {
	method			SF_INHERITED_TYPE
	primitive		SF_DOUBLE_TYPE
      }
      complexity	      SF_COMPLEX_INHERITED
    }
    dataType		    "Inherit: Same as Simulink"
  }
  data {
    id			    7
    ssIdNumber		    5
    name		    "y"
    linkNode		    [2 6 8]
    scope		    OUTPUT_DATA
    machine		    1
    props {
      array {
	size			"-1"
      }
      type {
	method			SF_INHERITED_TYPE
	primitive		SF_DOUBLE_TYPE
      }
      complexity	      SF_COMPLEX_INHERITED
      frame		      SF_FRAME_NO
    }
    dataType		    "Inherit: Same as Simulink"
  }
  data {
    id			    8
    ssIdNumber		    6
    name		    "C"
    linkNode		    [2 7 9]
    scope		    INPUT_DATA
    machine		    1
    props {
      array {
	size			"-1"
      }
      type {
	method			SF_INHERITED_TYPE
	primitive		SF_DOUBLE_TYPE
	isSigned		1
	wordLength		"16"
      }
      complexity	      SF_COMPLEX_INHERITED
      frame		      SF_FRAME_INHERITED
    }
    dataType		    "Inherit: Same as Simulink"
  }
  data {
    id			    9
    ssIdNumber		    7
    name		    "e"
    linkNode		    [2 8 0]
    scope		    INPUT_DATA
    machine		    1
    props {
      array {
	size			"-1"
      }
      type {
	method			SF_INHERITED_TYPE
	primitive		SF_DOUBLE_TYPE
	isSigned		1
	wordLength		"16"
      }
      complexity	      SF_COMPLEX_INHERITED
      frame		      SF_FRAME_INHERITED
    }
    dataType		    "Inherit: Same as Simulink"
  }
  instance {
    id			    10
    name		    "Branche/MATLAB Function"
    machine		    1
    chart		    2
  }
  target {
    id			    11
    name		    "sfun"
    description		    "Default Simulink S-Function Target."
    machine		    1
    linkNode		    [1 0 0]
  }
}
